From 43ad46cdac1e4d604a3b8805a9563b39981d7646 Mon Sep 17 00:00:00 2001
From: Jens Arnold <amiconn@rockbox.org>
Date: Mon, 20 Oct 2008 07:10:14 +0000
Subject: Fix title case in a section header, switch a sentence order for
 recorders to be more logical, and add a note about 8MB-modded boxes.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@18842 a1c6a512-1295-4272-9138-f99709370657
---
 manual/advanced_topics/archos-flashing.tex | 18 ++++++++++++------
 1 file changed, 12 insertions(+), 6 deletions(-)

(limited to 'manual/advanced_topics/archos-flashing.tex')

diff --git a/manual/advanced_topics/archos-flashing.tex b/manual/advanced_topics/archos-flashing.tex
index 5b730820d2..110272a4c3 100644
--- a/manual/advanced_topics/archos-flashing.tex
+++ b/manual/advanced_topics/archos-flashing.tex
@@ -48,7 +48,7 @@ outside, even if the flash ROM is completely erased.
 If the first $\approx$2KB of the flash ROM are flashed ok, \emph{Minimon} can
 be used for the same purpose.
 
-\subsection{Terminology and Basic operation}
+\subsection{Terminology and Basic Operation}
 
 \begin{description}
 \item[Firmware:] The flash ROM contents as a whole.
@@ -114,15 +114,15 @@ a safe place.
 \item Unzip the flash package to the root of your \dap.
   \nopt{ondio}{This will extract two files to the root,
     \fname{firmware\_{\textless}model{\textgreater}.bin} and
-    \fname{firmware\_{\textless}model{\textgreater}\_norom.bin}. The flash
-    plugin will select the correct one for your \dap.
+    \fname{firmware\_{\textless}model{\textgreater}\_norom.bin}.
+    \opt{recorder,recorderv2fm}{(The {\textless}model{\textgreater} part is
+      slighty different from that in the .zip file name.)
+    }
+    The flash plugin will select the correct one for your \dap.
   }
   \opt{ondio}{This will extract one file to the root,
     \fname{firmware\_{\textless}model{\textgreater}.bin}.
   }
-  \opt{recorder,recorderv2fm}{(The {\textless}model{\textgreater} part is
-    slighty different from that in the .zip file name.)
-  }
   Now safely disconnect USB.
 \item
   \nopt{ondio}{Make sure your batteries are in good shape and fully charged.}
@@ -150,6 +150,12 @@ a safe place.
   root of your \dap.
 }
 
+\note{There are no separate flash packages for {\dap}s modified to have 8MB
+  of RAM. You need to use the corresponding package for non-modified
+  \playertype. You should then install a rockbox image that makes use of all
+  available RAM as described in the following section.
+}
+
 \subsection{Updating the Rockbox Image in Flash}
 
 When Rockbox is booted from flash, it does not check for an updated firmware
-- 
cgit v1.2.3

