From a5501d68ccbb2f9690cb8d6a83b17b4bb204aa6c Mon Sep 17 00:00:00 2001
From: Jens Arnold <amiconn@rockbox.org>
Date: Tue, 24 Mar 2009 01:11:44 +0000
Subject: Bump flash image version and adapt flashing documentation.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@20510 a1c6a512-1295-4272-9138-f99709370657
---
 manual/advanced_topics/archos-flashing.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/advanced_topics/archos-flashing.tex')

diff --git a/manual/advanced_topics/archos-flashing.tex b/manual/advanced_topics/archos-flashing.tex
index 110272a4c3..e2e1f4f2ce 100644
--- a/manual/advanced_topics/archos-flashing.tex
+++ b/manual/advanced_topics/archos-flashing.tex
@@ -59,7 +59,7 @@ The replacement firmware contains a bootloader and two images. The first image
 is the \emph{permanent} rescue software, to be used in case something is wrong
 with the second (main) image. In current firmware files this first image
 contains \emph{Bootbox} (see wiki for details). The second image is what is
-booted by default. The current firmware files contain a copy of Rockbox 3.0.1
+booted by default. The current firmware files contain a copy of Rockbox 3.2
 in the main image. It can easily be updated/replaced later.
 
 The bootloader allows to select which image to run. Pressing
@@ -110,7 +110,7 @@ a safe place.
 \item Download the correct package for your \dap\ from
   \url{http://download.rockbox.org/bootloader/archos/}. It is named
   \fname{flash-{\textless}model{\textgreater}-{\textless}version{\textgreater}.zip}.
-  The current packages are v2.
+  The current packages are v3.
 \item Unzip the flash package to the root of your \dap.
   \nopt{ondio}{This will extract two files to the root,
     \fname{firmware\_{\textless}model{\textgreater}.bin} and
-- 
cgit v1.2.3

