From e8c72b68917b064c6ec7b87d46b4ee59faea7ffb Mon Sep 17 00:00:00 2001
From: Alexander Levin <al.le@rockbox.org>
Date: Sun, 9 May 2010 18:33:31 +0000
Subject: Use typographic quotation marks -- correct more places

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25917 a1c6a512-1295-4272-9138-f99709370657
---
 manual/advanced_topics/archos-flashing.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'manual/advanced_topics/archos-flashing.tex')

diff --git a/manual/advanced_topics/archos-flashing.tex b/manual/advanced_topics/archos-flashing.tex
index 4f6c622cd4..c6209be2cf 100644
--- a/manual/advanced_topics/archos-flashing.tex
+++ b/manual/advanced_topics/archos-flashing.tex
@@ -42,7 +42,7 @@ There's an ultimate safety net to bring back boxes with even completely
 garbled flash content: the \emph{UART} boot mod, which in turn requires the
 \emph{serial} mod. With that it's possible to reflash independently from the
 outside, even if the flash ROM is completely erased.
-\nopt{ondio}{This won't work if you have one of the rare "ROMless" boxes. These
+\nopt{ondio}{This won't work if you have one of the rare ``ROMless'' boxes. These
   have no boot ROM and boot directly from flash.
 }
 If the first $\approx$2KB of the flash ROM are flashed ok, \emph{Minimon} can
@@ -78,7 +78,7 @@ screen. To get out of it, perform a hardware shutdown of your \dap.
 You only need to perform this procedure the first time you flash your
 \playertype. You may also want to perform it in case the update procedure for
 the second image recommends it. In the latter case do not perform the steps
-listed under "Preparation".
+listed under ``Preparation''.
 
 \subsubsection{Preparation}
 
@@ -87,10 +87,10 @@ listed under "Preparation".
   \setting{System $\rightarrow$ Debug (Keep Out!) $\rightarrow$ View HW
   Info}. 
   \opt{lcd_charcell}{Cycle through the displayed values with \ButtonRight /
-    \ButtonLeft\ until "Flash:" is displayed. If it shows question marks,
+    \ButtonLeft\ until ``Flash:'' is displayed. If it shows question marks,
   }
-  \opt{lcd_bitmap}{Check the values in the line starting with "Flash:". If it
-    shows question marks after "M=" and "D=",
+  \opt{lcd_bitmap}{Check the values in the line starting with ``Flash:''. If it
+    shows question marks after ``M='' and ``D='',
   }
   you're out of luck, your \dap\ is not flashable without modifying the
   hardware. You can stop here. Sorry.
-- 
cgit v1.2.3

