From 66fa5b578904f7df61293d6ce5c08966b5db13db Mon Sep 17 00:00:00 2001
From: Björn Stenberg <bjorn@haxx.se>
Date: Mon, 7 Dec 2009 09:03:11 +0000
Subject: Rename targets to be consistent in all places. (FS #10819)

git-svn-id: svn://svn.rockbox.org/rockbox/branches/v3_4@23881 a1c6a512-1295-4272-9138-f99709370657
---
 manual/advanced_topics/main.tex | 14 +++++++-------
 1 file changed, 7 insertions(+), 7 deletions(-)

(limited to 'manual/advanced_topics/main.tex')

diff --git a/manual/advanced_topics/main.tex b/manual/advanced_topics/main.tex
index 53bb984f2e..23748da18a 100644
--- a/manual/advanced_topics/main.tex
+++ b/manual/advanced_topics/main.tex
@@ -213,7 +213,7 @@ all the tags that are available.
   the last number giving the colour depth in bits) when
   designing your own WPS, or if you use a WPS designed for another target.
   \opt{HAVE_REMOTE_LCD}{The resolution of the remote is
-  \opt{h100,h300}{128x64x1}\opt{x5,m5}{128x96x2} pixels.}}
+  \opt{iriverh100,iriverh300}{128x64x1}\opt{iaudiox5,iaudiom5}{128x96x2} pixels.}}
 
 \nopt{lcd_charcell}{
 \subsubsection{\label{ref:Viewports}Viewports}
@@ -554,7 +554,7 @@ Example of a configuration file:
 \end{description}
 
 \section{\label{ref:FirmwareLoading}Firmware Loading}
-\opt{player,recorder,recorderv2fm,ondio}{
+\opt{archosplayer,archosrecorder,archosrecorderv2fm,ondio}{
   When your \dap{} powers on, it loads the Archos firmware in ROM, which
   automatically checks your \daps{} root directory for a file named 
   \firmwarefilename. Note that Archos firmware can only read the first 
@@ -567,14 +567,14 @@ Example of a configuration file:
 \subsection{\label{ref:using_rolo}Using ROLO (Rockbox Loader)}
 Rockbox is able to load and start another firmware file without rebooting. 
 You just ``play'' a file with the extension %
-\opt{recorder,recorderv2fm,ondio}{\fname{.ajz}.} %
-\opt{player}{\fname{.mod}.} %
-\opt{h100,h300}{\fname{.iriver}.} %
+\opt{archosrecorder,archosrecorderv2fm,ondio}{\fname{.ajz}.} %
+\opt{archosplayer}{\fname{.mod}.} %
+\opt{iriverh100,iriverh300}{\fname{.iriver}.} %
 \opt{ipod}{\fname{.ipod}.} %
 \opt{iaudio}{\fname{.iaudio}.} %
-\opt{sansa,h10,h10_5gb}{\fname{.mi4}.} %
+\opt{sansa,iriverh10,iriverh10_5gb}{\fname{.mi4}.} %
 \opt{sansaAMS}{\fname{.sansa}.} %
-\opt{gigabeatf,gigabeats}{\fname{.gigabeat}.} %
+\opt{gigabeatfx,gigabeats}{\fname{.gigabeat}.} %
 This can be used to test new firmware versions without deleting your
 current version.
 
-- 
cgit v1.2.3

