From 963e979e6c1abeb81d1f4e1a2cca92ed220f0a67 Mon Sep 17 00:00:00 2001
From: Johannes Rauh <johnbthetenth@gmail.com>
Date: Thu, 20 Aug 2020 15:52:53 +0200
Subject: Manual: add Multiboot for Sansa E200

Change-Id: I89d0881face9952184f49f28740896ead3c2dfb5
---
 manual/advanced_topics/main.tex | 1 +
 1 file changed, 1 insertion(+)

(limited to 'manual/advanced_topics/main.tex')

diff --git a/manual/advanced_topics/main.tex b/manual/advanced_topics/main.tex
index 997850a6fd..66793a8d24 100755
--- a/manual/advanced_topics/main.tex
+++ b/manual/advanced_topics/main.tex
@@ -684,6 +684,7 @@ current version.
   \opt{fuzeplus}{\renewcommand*{\redirectext}{fuze+}}
   \opt{clipplus}{\renewcommand*{\redirectext}{clip+}}
   \opt{clipzip}{\renewcommand*{\redirectext}{clipzip}}
+  \opt{e200}{\renewcommand*{\redirectext}{e200}}
 
   Using a specially crafted redirect file combined with special firmware builds
   that allow the boot drive to be passed from the bootloader, some devices can
-- 
cgit v1.2.3

