From a8b5589523a0be2f26a22607e5c0e12382a64f4e Mon Sep 17 00:00:00 2001
From: Szymon Dziok <b0hoon@o2.pl>
Date: Wed, 15 Oct 2014 16:23:34 +0200
Subject: Manual for the Samsung YH920/YH925.

Change-Id: I2db0023cae585e9c9517da9ed2e9de6195081ce2
---
 manual/advanced_topics/main.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/advanced_topics/main.tex')

diff --git a/manual/advanced_topics/main.tex b/manual/advanced_topics/main.tex
index 032841edd2..687c418e4c 100644
--- a/manual/advanced_topics/main.tex
+++ b/manual/advanced_topics/main.tex
@@ -622,7 +622,7 @@ Example of a configuration file:
   in the \dap{} and resets all settings to their default values. 
   
   \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_X5_PAD,SANSA_E200_PAD,SANSA_C200_PAD%
-      ,PBELL_VIBE500_PAD}{
+      ,PBELL_VIBE500_PAD,SAMSUNG_YH92X_PAD}{
       \note{You can also reset all settings to their default 
       values by turning off the \dap, turning it back on, and holding the
       \ButtonRec{} button immediately after the \dap{} turns on.}
@@ -680,7 +680,7 @@ You just ``play'' a file with the extension %
 \opt{iriverh100,iriverh300}{\fname{.iriver}.} %
 \opt{ipod}{\fname{.ipod}.} %
 \opt{iaudio}{\fname{.iaudio}.} %
-\opt{sansa,iriverh10,iriverh10_5gb,mrobe100,vibe500}{\fname{.mi4}.} %
+\opt{sansa,iriverh10,iriverh10_5gb,mrobe100,vibe500,samsungyh}{\fname{.mi4}.} %
 \opt{sansaAMS,fuzeplus}{\fname{.sansa}.} %
 \opt{gigabeatf,gigabeats}{\fname{.gigabeat}.} %
 This can be used to test new firmware versions without deleting your
-- 
cgit v1.2.3

