From f498d53d72007124049cf72ccccf3435abb097fe Mon Sep 17 00:00:00 2001
From: Dominik Riebeling <Dominik.Riebeling@gmail.com>
Date: Sun, 7 Dec 2008 23:00:15 +0000
Subject: Rename h100 manual name "h1xx" to "h100" to be in line with other
 players.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19361 a1c6a512-1295-4272-9138-f99709370657
---
 manual/advanced_topics/main.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/advanced_topics/main.tex')

diff --git a/manual/advanced_topics/main.tex b/manual/advanced_topics/main.tex
index 6247fe3a2f..a567e82926 100644
--- a/manual/advanced_topics/main.tex
+++ b/manual/advanced_topics/main.tex
@@ -116,7 +116,7 @@ all the tags that are available.
   the last number giving the colour depth in bits) when
   designing your own WPS, or if you use a WPS designed for another target.
   \opt{HAVE_REMOTE_LCD}{The resolution of the remote is
-  \opt{h1xx,h300}{128x64x1}\opt{x5}{128x96x2} pixels.}}
+  \opt{h100,h300}{128x64x1}\opt{x5}{128x96x2} pixels.}}
 
 \subsubsection{Conditional Tags}
 
@@ -411,7 +411,7 @@ Rockbox is able to load and start another firmware file without rebooting.
 You just ``play'' a file with the extension %
 \opt{recorder,recorderv2fm,ondio}{\fname{.ajz}.} %
 \opt{player}{\fname{.mod}.} %
-\opt{h1xx,h300}{\fname{.iriver}.} %
+\opt{h100,h300}{\fname{.iriver}.} %
 \opt{ipod}{\fname{.ipod}.} %
 \opt{iaudio}{\fname{.iaudio}.} %
 \opt{sansa,h10,h10_5gb}{\fname{.mi4}.} %
-- 
cgit v1.2.3

