From 4cd65b9d97e5fb172477b31d3dc5bc136cc6950b Mon Sep 17 00:00:00 2001
From: "roman.artiukhin" <bahusdrive@gmail.com>
Date: Fri, 22 Dec 2023 13:40:54 +0200
Subject: Codecs: mp4: Disable SBR decoding for PP5002 - PP5022 platforms

Includes ipod video (5G) and earlier models, sansa c200 and others players not capable to decode AAC-HE.

Allows to play backward compatible files as AAC-LC.

Change-Id: Ic9f5c0f255d9a4308c3414d402f8f27f4328ca94
---
 manual/appendix/file_formats.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'manual/appendix/file_formats.tex')

diff --git a/manual/appendix/file_formats.tex b/manual/appendix/file_formats.tex
index c40a7d35ae..dd12993d36 100644
--- a/manual/appendix/file_formats.tex
+++ b/manual/appendix/file_formats.tex
@@ -86,10 +86,10 @@
         & \fname{.adx}
         & Encrypted ADX is not supported.\\
     Advanced Audio Coding
-        & \fname{.m4a}, \fname{.m4b}, \fname{.mp4}, \fname{.rm}, \fname{.ra}, \fname{.rmvb}
-        \nopt{clipv1,c200v2}{
+        & \fname{.aac}, \fname{.m4a}, \fname{.m4b}, \fname{.mp4}, \fname{.rm}, \fname{.ra}, \fname{.rmvb}
+        \opt{codec_aac_he}{
             & Supports AAC-LC, -HEv1, and -HEv2 profiles\\}
-        \opt{clipv1,c200v2}{ % low memory targets (CODEC_SIZE <= 512 KB)
+        \nopt{codec_aac_he}{ % low memory (CODEC_SIZE <= 512 KB) or slow cpu targets 
             & Supports AAC-LC profile\\}
     MPEG audio
         & \fname{.mpa}, \fname{.mpga}, \fname{.mp1}, \fname{.mp2}, \fname{.mp3}
@@ -122,7 +122,7 @@
         & \\
   \end{rbtabular}
 
-  \note{AAC-HE profiles might not play in realtime on all devices due to CPU
+  \note{AAC-HE profiles \opt{codec_aac_he}{might not play in realtime on all devices}\nopt{codec_aac_he}{are disabled on this device} due to CPU
   performance requirements.}
 
   \subsection{Lossless Codecs}
-- 
cgit v1.2.3

