From 37400f8d4decf2d5aee5abe5a1a08a1ec024306f Mon Sep 17 00:00:00 2001
From: Marc Guay <marcguay@rockbox.org>
Date: Mon, 14 Jul 2008 06:17:40 +0000
Subject: Revert most of r18029 as recording through line-in is possible on the
 H10, just not currently functional.  Leave the /nopt for line-in on the
 Sansas.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@18030 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/recording_settings.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/configure_rockbox/recording_settings.tex')

diff --git a/manual/configure_rockbox/recording_settings.tex b/manual/configure_rockbox/recording_settings.tex
index dcaad4760c..4607f0fa8a 100644
--- a/manual/configure_rockbox/recording_settings.tex
+++ b/manual/configure_rockbox/recording_settings.tex
@@ -73,7 +73,7 @@
   Choose the source of the recording. The options are: 
   \opt{recorder,recorderv2fm,h1xx}{\setting{SPDIF (digital)}, }%
   \nopt{ipodnano,ipodvideo}{\setting{Mic}, }%
-  \nopt{sansa,IRIVER_H10_PAD}{{\setting{Line In}}}. %
+  \nopt{sansa}{{\setting{Line In}}}. %
   \opt{radio}{For recording from the radio see \reference{ref:FMradio}.}
 
 \section{Channels}
-- 
cgit v1.2.3

