From e8c72b68917b064c6ec7b87d46b4ee59faea7ffb Mon Sep 17 00:00:00 2001
From: Alexander Levin <al.le@rockbox.org>
Date: Sun, 9 May 2010 18:33:31 +0000
Subject: Use typographic quotation marks -- correct more places

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25917 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/recording_settings.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/configure_rockbox/recording_settings.tex')

diff --git a/manual/configure_rockbox/recording_settings.tex b/manual/configure_rockbox/recording_settings.tex
index 78befa623f..3ab3966b70 100644
--- a/manual/configure_rockbox/recording_settings.tex
+++ b/manual/configure_rockbox/recording_settings.tex
@@ -193,7 +193,7 @@
     
   \item[Start Above.]
     The start threshold defines the minimal volume a sound must have to start the
-    recording. It is displayed numerically in the line "Start Above". Note that
+    recording. It is displayed numerically in the line ``Start Above''. Note that
     the unit of the threshold depends on the settings of the peak meter. (i.e.
     When the peak meter displays dB you can adjust the level in dB and when the
     peak meter is set to linear the threshold is displayed as percentage.) In the
@@ -216,7 +216,7 @@
     
   \item[Stop Below.]
     When the sound level drops below the stop threshold the recording is stopped.
-    It is displayed numerically in the line "Stop Below". Just like the start
+    It is displayed numerically in the line ``Stop Below''. Just like the start
     threshold the unit of the stop threshold depends on the settings of the peak
     meter. There's also a small triangular marker in the peak meter at the bottom
     of the screen. In contrast to the start threshold marker it points to the
-- 
cgit v1.2.3

