From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/configure_rockbox/sound_settings.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/configure_rockbox/sound_settings.tex')

diff --git a/manual/configure_rockbox/sound_settings.tex b/manual/configure_rockbox/sound_settings.tex
index 3ac346d256..caebd3c37c 100644
--- a/manual/configure_rockbox/sound_settings.tex
+++ b/manual/configure_rockbox/sound_settings.tex
@@ -502,7 +502,7 @@ change to customise your listening experience.
       \opt{GIGABEAT_PAD,GIGABEAT_S_PAD,SANSA_C200_PAD,MROBE100_PAD,SANSA_CLIP_PAD}{\ButtonPower}
       \opt{PBELL_VIBE500_PAD}{\ButtonCancel}
       \opt{SANSA_FUZEPLUS_PAD}{\ButtonBack}
-      \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
+      \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonPlay}
       \opt{touchscreen}{\TouchTopLeft
           \opt{COWON_D2_PAD}{/ \ButtonPower}}
           &
-- 
cgit v1.2.3

