From b43b4936a108e857d794264724ed7c6399bc5aac Mon Sep 17 00:00:00 2001
From: Marianne Arnold <pixelma@rockbox.org>
Date: Mon, 17 Jan 2011 18:30:18 +0000
Subject: Pick up the target rename completion in the manual started in r27823
 ... this time taking care of the Iriver targets. This fixes a few issues with
 wrongly in- or excluded parts (e.g. pacbox missing from the H100 manual,
 invadrox wrongly included in the small H10 manual as the plugin's main.tex
 already used the new names without making sure they are there). If possible
 replace 'target name' \opts with sensible feature \opts. Fix small mistakes
 and break too long lines discovered along the way.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@29075 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/sound_settings.tex | 18 +++++++++---------
 1 file changed, 9 insertions(+), 9 deletions(-)

(limited to 'manual/configure_rockbox/sound_settings.tex')

diff --git a/manual/configure_rockbox/sound_settings.tex b/manual/configure_rockbox/sound_settings.tex
index 406cc3679b..3e71c45cae 100644
--- a/manual/configure_rockbox/sound_settings.tex
+++ b/manual/configure_rockbox/sound_settings.tex
@@ -10,7 +10,7 @@ change to customise your listening experience.
   where 0~dB is a reference that indicates the maximum volume that the \dap{}
   can produce without possible distortion (clipping). All values lower than
   this reference will be negative and yield a progressively softer volume.
-  \nopt{h100,h300,ondavx777}{%
+  \nopt{iriverh100,iriverh300,ondavx777}{%
       Values higher than 0~dB are available and can be used to raise the
       volume more than would otherwise be possible. These volume levels will
       ordinarily lead to distorted sound, but might work nicely for music that has
@@ -19,12 +19,12 @@ change to customise your listening experience.
   The volume can be adjusted from a
   \opt{player}{minimum of -78~dB to a maximum of +18~dB.}%
   \opt{recorder,recorderv2fm,ondio}{minimum of -100~dB to a maximum of +12~dB.}%
-  \opt{h100,h300}{minimum of -84~dB to a maximum of 0~dB.}%
+  \opt{iriverh100,iriverh300}{minimum of -84~dB to a maximum of 0~dB.}%
   \opt{iaudiom3,iaudiom5,iaudiox5,ipod3g,ipod4g,gigabeatf,mrobe100,mpiohd200}{%
       minimum of -73~dB to a maximum of +6~dB.}%
   \opt{ipodnano}{minimum of -72~dB to a maximum of +6~dB.}%
   \opt{ipodvideo,cowond2}{minimum of -89~dB to a maximum of +6~dB.}%
-  \opt{ipodnano2g,ipodcolor,ipod1g2g,h10,h10_5gb,sansa,sansaAMS}{minimum of 
+  \opt{ipodnano2g,ipodcolor,ipod1g2g,iriverh10,iriverh10_5gb,sansa,sansaAMS}{minimum of 
       -74~dB to a maximum of +6~dB.}%
   \opt{gigabeats}{minimum of -90~dB to a maximum of +6~dB.}%
   \opt{gigabeatf,vibe500}{minimum of -74~dB to a maximum of +6~dB.}%
@@ -35,16 +35,16 @@ change to customise your listening experience.
 \nopt{gigabeats}{  
 \section{Bass}
   This setting emphasises
-  \nopt{h100,h300}{or suppresses}
+  \nopt{iriverh100,iriverh300}{or suppresses}
   the lower (bass) frequencies in the sound. A value of 0~dB means that bass
   sounds are unaltered (flat response).
   \opt{masd}{The minimum setting is -15~dB and the maximum is 15~dB.}%
   \opt{masf}{The minimum setting is -12~dB and the maximum is 12~dB.}%
-  \opt{h100,h300}{The minimum setting is 0~dB and the maximum is 24~dB.}%
+  \opt{iriverh100,iriverh300}{The minimum setting is 0~dB and the maximum is 24~dB.}%
   \opt{ipodnano,ipodnano2g,ipodcolor,mpiohd200}{%
       The minimum setting is -6~dB and the maximum is 9~dB.}%
   \opt{ipodvideo}{The minimum setting is -12~dB and the maximum is 12~dB.}%
-  \opt{iaudiom3,iaudiom5,iaudiox5,sansa,sansaAMS,h10,h10_5gb,vibe500}{%
+  \opt{iaudiom3,iaudiom5,iaudiox5,sansa,sansaAMS,iriverh10,iriverh10_5gb,vibe500}{%
       The minimum setting is -24~dB and the maximum is 24~dB.}
 
 \opt{ipodvideo}{
@@ -57,16 +57,16 @@ change to customise your listening experience.
 
 \section{Treble}
   This setting emphasises
-  \nopt{h100,h300}{or suppresses}
+  \nopt{iriverh100,iriverh300}{or suppresses}
   the higher (treble) frequencies in the sound. A value of 0~dB means that
   treble sounds are unaltered (flat response).
   \opt{masd}{The minimum setting is -15~dB and the maximum is 15~dB.}%
   \opt{masf}{The minimum setting is -12~dB and the maximum is 12~dB.}%
-  \opt{h100,h300}{The minimum setting is 0~dB and the maximum is 6~dB.}%
+  \opt{iriverh100,iriverh300}{The minimum setting is 0~dB and the maximum is 6~dB.}%
   \opt{ipodnano,ipodnano2g,ipodcolor,mpiohd200}{%
       The minimum setting is -6~dB and the maximum is 9~dB.}%
   \opt{ipodvideo}{The minimum setting is -12~dB and the maximum is 12~dB.}%
-  \opt{iaudiom3,iaudiom5,iaudiox5,sansa,sansaAMS,h10,h10_5gb,vibe500}{%
+  \opt{iaudiom3,iaudiom5,iaudiox5,sansa,sansaAMS,iriverh10,iriverh10_5gb,vibe500}{%
       The minimum setting is -24~dB and the maximum is 24~dB.}
 
 \opt{ipodvideo}{
-- 
cgit v1.2.3

