From 4add1af7637e34567c5dedd6acfee3ccc4c0e8ac Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Tue, 6 Jan 2009 11:35:47 +0000
Subject: A couple of small fixes for the gigabeat s manual.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19698 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index 8c7d93ffe2..a6c62021a8 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -27,6 +27,8 @@
       \opt{ipod3g}{630mAh}%
       \opt{ipod1g2g}{1200mAh}%
       \opt{m5,x5}{950mAh}%
+      \opt{gigabeatf}{2000mAh}%
+      \opt{gigabeats}{700mAh}%
       , which is the capacity value for the standard
       \opt{archos}{batteries}\nopt{archos}{battery} shipped with the \dap.
         Rockbox uses this value to estimate remaining battery life for the
@@ -47,7 +49,6 @@
         ``Alkaline'' or ``NiMH''.}
 
       \opt{usb_charging}{
-%TODO: check where it is working correctly (except H300) and append the option to the respective platform file
       \item [Charge During USB Connection: ]This option lets you control whether
         the \dap{} should charge during the USB connection and hence draw the
         full 500mA. Turning it \setting{Off} is recommended if the dap{} is
-- 
cgit v1.2.3

