From 619ffcb0e60a21aaed3500f0ef0cd606c47225f1 Mon Sep 17 00:00:00 2001
From: Tomer Shalev <shalev.tomer@gmail.com>
Date: Wed, 30 Sep 2009 14:16:49 +0000
Subject: Since we have usb_hid in feature.txt we don't need a seperate
 UseOption in the platform file for the manual (thanks for pixelma for
 noticing)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@22858 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index 83146b69c0..3c70f4a313 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -182,7 +182,7 @@ this option \setting{On}. If it is not required, then turning this setting
       Changes the brightness of the button lights.
   }
 }
-\opt{USB_ENABLE_HID}{
+\opt{usb_hid}{
   \subsection{USB keypad Mode}
     This setting control the keypad mode when the \dap{} is attached to a
     computer through USB. The \dap{} registers itself as a USB keyboard (in
@@ -253,7 +253,6 @@ this option \setting{On}. If it is not required, then turning this setting
                 ,IRIVER_H10_PAD,IPOD_4G_PAD,IPOD_3G_PAD,IPOD_1G2G_PAD%
                 ,MROBE100_PAD}
               {\ButtonLeft / \ButtonRight}
-            \opt{SANSA_E200_PAD}{\ButtonMenu}
             \opt{HAVEREMOTEKEYMAP}{
               &
               \opt{GIGABEAT_RC_PAD}{\ButtonRCRew / \ButtonRCFF}%
-- 
cgit v1.2.3

