From 6a96037d09c99041bae87ae7c7a5189adafd7408 Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Sun, 9 May 2010 21:03:30 +0000
Subject: Add non-breaking spaces to mA, mAh, MB and GB. Add playertype for
 iPod Video when describing the different variants.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25921 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/gigabeats_install.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/getting_started/gigabeats_install.tex')

diff --git a/manual/getting_started/gigabeats_install.tex b/manual/getting_started/gigabeats_install.tex
index deb260bfe4..5952c167db 100644
--- a/manual/getting_started/gigabeats_install.tex
+++ b/manual/getting_started/gigabeats_install.tex
@@ -18,7 +18,7 @@ only possible to connect the \dap{} to a PC in ``MTP mode'', which hides
 the actual content of your \daps{} disk and provides restricted access
 to its contents.
 In reality, the \daps{} hard disk contains two partitions, a small
-(150MB) ``firmware partition'' containing the \daps{} firmware (operating
+(150~MB) ``firmware partition'' containing the \daps{} firmware (operating
 system), and a second ``data partition'' containing your media files. The main
 firmware file in the bootloader partition is called \fname{nk.bin}, and
 this is the file that is loaded into RAM (by the \daps{} ROM-based
-- 
cgit v1.2.3

