From a2d8212a84a30e2cb293dfe6e6a10a7cf1ac0cdf Mon Sep 17 00:00:00 2001
From: Michael Chicoine <mc2739@gmail.com>
Date: Mon, 30 Nov 2009 01:08:15 +0000
Subject: Gigibeat S Manual - redo r23795 to look like it was originally meant
 to look.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@23797 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/gigabeats_install.tex | 18 ++++++++++++------
 1 file changed, 12 insertions(+), 6 deletions(-)

(limited to 'manual/getting_started/gigabeats_install.tex')

diff --git a/manual/getting_started/gigabeats_install.tex b/manual/getting_started/gigabeats_install.tex
index 67c8aa9c5f..deb260bfe4 100644
--- a/manual/getting_started/gigabeats_install.tex
+++ b/manual/getting_started/gigabeats_install.tex
@@ -35,7 +35,8 @@ bootloader) and executed when your \dap{} is powered on.
 and then perform one of the following, depending on whether you want single
 or dual-boot.
 
-\item Single Boot. Run \fname{beastpatcher.exe}. You should see some
+\begin{description}
+\item [Single Boot.] Run \fname{beastpatcher.exe}. You should see some
 information displayed about
 your \dap{} and a message asking you if you wish to install the Rockbox
 bootloader. Press i followed by ENTER, and beastpatcher will
@@ -43,7 +44,7 @@ install the bootloader. After a short time you should see the message
 ``[INFO] Bootloader installed successfully''. Press ENTER again to exit
 beastpatcher.
 
-\item Dual Boot. Inside the \fname{MESV12US.zip} file you downloaded earlier
+\item [Dual Boot.] Inside the \fname{MESV12US.zip} file you downloaded earlier
 you should find an \fname{.iso} file.  Using e.g. 7zip
 (\url{http://www.7-zip.org} you can extract an \fname{.exe} file from this
 \fname{.iso} file.  Using 7zip again, extract the \playerman{} firmware file
@@ -58,6 +59,7 @@ to this directory, and then type the following commands:
 After a short time you should see the message
 ``[INFO] Bootloader installed successfully''. Press ENTER again to exit
 beastpatcher.
+\end{description}
 
 \item After a successful installation, you need to disconnect your \dap{} from
 USB, and then immediately reconnect it. It should reboot then enter the Rockbox
@@ -74,7 +76,8 @@ computer as a standard USB Mass Storage device.
 and then perform one of the following,
 depending on whether you want single or dual-boot.
 
-\item Single Boot. Double-click on the beastpatcher icon. You can also
+\begin{description}
+\item [Single Boot.] Double-click on the beastpatcher icon. You can also
 drag the beastpatcher icon to a location on your hard drive and launch
 it from the Terminal. If all has gone well, you should see some 
 information displayed about your \dap{} and a message asking you if you 
@@ -84,7 +87,7 @@ should see the message ``[INFO] Bootloader installed successfully''
 followed by some error messages that you can safely ignore. Press 
 ENTER again to exit beastpatcher and then quit the Terminal application.
 
-\item Dual Boot. Inside the \fname{MESV12US.zip} file you downloaded earlier
+\item [Dual Boot.] Inside the \fname{MESV12US.zip} file you downloaded earlier
 you should find an \fname{.iso} file.  Using e.g. 7zip
 (\url{http://www.7-zip.org} you can extract an \fname{.exe} file from this
 \fname{.iso} file.  Using 7zip again, extract the \playerman{} firmware file
@@ -95,6 +98,7 @@ following command:
 \begin{code} 
     ./beastpatcher -d nk.bin
 \end{code}
+\end{description}
 
 \item After a successful installation, your \dap{} will immediately turn off.
 Turn it on again, and (because it is still connected to your Mac)
@@ -117,7 +121,8 @@ steps will assume you have saved it in your home directory.
 \item Attach your \dap{} to your computer and then perform one of the following,
 depending on whether you want single or dual-boot.
 
-\item Single Boot. Open up a terminal window and type the following commands:
+\begin{description}
+\item [Single Boot.] Open up a terminal window and type the following commands:
 
 \begin{code} 
     cd $HOME
@@ -132,7 +137,7 @@ bootloader. After a short time you should see the message ``[INFO] Bootloader
 installed successfully'' followed by some error
 messages that you can safely ignore. Press ENTER again to exit beastpatcher.
 
-\item Dual Boot. Inside the \fname{MESV12US.zip} file you downloaded earlier
+\item [Dual Boot.] Inside the \fname{MESV12US.zip} file you downloaded earlier
 you should find an \fname{.iso} file.  Using e.g. 7zip
 (\url{http://www.7-zip.org} you can extract an \fname{.exe} file from this
 \fname{.iso} file.  Using 7zip again, extract the \playerman{} firmware file
@@ -150,6 +155,7 @@ After a short time you should see the message
 ``[INFO] Bootloader installed successfully'' followed by some error
 messages that you can safely ignore. Press ENTER again to exit
 beastpatcher.
+\end{description}
 
 \item After a successful installation, your \dap{} will immediately turn off.
 Turn it on again, and (because it is still connected to your PC)
-- 
cgit v1.2.3

