From 8f05109b36d3b2fc446ee695be8558a768e4e837 Mon Sep 17 00:00:00 2001
From: Barry Wardell <rockbox@barrywardell.net>
Date: Tue, 20 Mar 2007 23:44:16 +0000
Subject: Update H10 installation instructions now that we support booting
 encrypted mi4s.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@12868 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/h10_install.tex | 7 +++----
 1 file changed, 3 insertions(+), 4 deletions(-)

(limited to 'manual/getting_started/h10_install.tex')

diff --git a/manual/getting_started/h10_install.tex b/manual/getting_started/h10_install.tex
index b4ab3516c8..498c9f1fad 100644
--- a/manual/getting_started/h10_install.tex
+++ b/manual/getting_started/h10_install.tex
@@ -15,7 +15,7 @@ It is possible to force a MTP \playertype{} to start up in UMS mode using the fo
   \item Continue holding \ButtonRight{} until the USB Connected screen appears.
   \item The \dap{} will now appear as a regular disk on your computer.
 \end{enumerate}
-\note{Once Rockbox has been installed, when you shut down your \dap{} from Rockbox it will totally power the player off, so step 1 is no longer necessary.}
+\note{Once Rockbox has been installed, when you shut down your \dap{} from Rockbox it will totally power the player off so step 1 is no longer necessary.}
 
 \subsubsection{Installation}
 \begin{enumerate}
@@ -27,11 +27,10 @@ It is possible to force a MTP \playertype{} to start up in UMS mode using the fo
       \item \url{http://download.rockbox.org/bootloader/iriver/H10_5GB-MTP/H10.mi4} if it is MTP.
     \end{itemize}}
   \item Connect your \playertype{} to the computer using UMS mode and the UMS trick\opt{h10_5gb}{ if necessary}.
-  \item Make a backup of the \opt{h10}{\fname{H10\_20GC.mi4}}\opt{h10_5gb}{\fname{H10.mi4}} file in the \fname{System} directory on your \playertype{}.
+  \item Rename the \opt{h10}{\fname{H10\_20GC.mi4}}\opt{h10_5gb}{\fname{H10.mi4}} file to \fname{OF.mi4} in the \fname{System} directory on your \playertype{}.
     \opt{h10_5gb}{\note{If you have a Pure model \playertype{} (which doesn't have a FM radio) it is possible that this file will be called \fname{H10EMP.mi4} instead. If so, rename the \fname{H10.mi4} you downloaded in step 1 to \fname{H10EMP.mi4}.}}
     \note{You should keep a safe backup of this file for use if you ever wish to switch back to the \playerman{} firmware.}
     \note{If you can't see the \fname{System} directory, you will need to make sure your operating system is configured to show hidden files and folders.}
 
   \item Copy the \opt{h10}{\fname{H10\_20GC.mi4}}\opt{h10_5gb}{\fname{H10.mi4} (or \fname{H10EMP.mi4} if you have a \playertype{} Pure)} file you downloaded to the System directory on your \dap{}.
-\end{enumerate}
-Now proceed with installing the firmware itself.
\ No newline at end of file
+\end{enumerate}
\ No newline at end of file
-- 
cgit v1.2.3

