From f8e2f3e08d779092cf7d3f26f369c0941edf9349 Mon Sep 17 00:00:00 2001
From: Martin Arver <martin.arver@gmail.com>
Date: Tue, 17 Oct 2006 12:18:51 +0000
Subject: Fix for more consistent and proper British English. (-ize/-ise etc)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@11246 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/h10_install.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'manual/getting_started/h10_install.tex')

diff --git a/manual/getting_started/h10_install.tex b/manual/getting_started/h10_install.tex
index cc804f008a..36a36d8ec4 100755
--- a/manual/getting_started/h10_install.tex
+++ b/manual/getting_started/h10_install.tex
@@ -4,7 +4,7 @@ The \playertype{} can be connected to a computer in two different modes:
   \item Universal Mass Storage (UMS): In this mode, it will appear on your computer as a regular disk. This mode works with all major operating systems, including Windows, Linux and Mac OS X.
   \item Media Transfer Protocol (MTP): In this mode, it will appear on your computer as a Media Device. MTP was created by Microsoft for use with DAPs and only works with Windows XP and Media Player 10.
 \end{itemize}
-The \playerlongtype{} is \opt{h10}{only available as a MTP device, but}\opt{h10_5gb}{available as both a MTP and as a UMS device, depending on where and when you bought it. You can tell which you have by how it appears when you conect it to a computer. If it appears as a regular disk then it is UMS. If it appears as a Media Device on Windows XP, or if it doesn't appear at all on other operating systems, then it is MTP. Even if you have a MTP \dap{}, it} can be forced into UMS mode using the UMS trick.
+The \playerlongtype{} is \opt{h10}{only available as a MTP device, but}\opt{h10_5gb}{available as both a MTP and as a UMS device, depending on where and when you bought it. You can tell which you have by how it appears when you connect it to a computer. If it appears as a regular disk then it is UMS. If it appears as a Media Device on Windows XP, or if it doesn't appear at all on other operating systems, then it is MTP. Even if you have a MTP \dap{}, it} can be forced into UMS mode using the UMS trick.
 
 \subsubsection{UMS mode and the UMS trick}
 It is possible to force a MTP \playertype{} to start up in UMS mode using the following procedure:
@@ -28,9 +28,9 @@ It is possible to force a MTP \playertype{} to start up in UMS mode using the fo
     \end{itemize}}
   \item Connect your \playertype{} to the computer using UMS mode and the UMS trick\opt{h10_5gb}{ if necessary}.
   \item Make a backup of the \opt{h10}{\fname{H10\_20GC.mi4}}\opt{h10_5gb}{\fname{H10.mi4}} file in the \fname{System} directory on your \playertype{}.
-    \opt{h10_5gb}{\note{If you have a Pure model \playertype{} (which doesn't have a FM radio) it is possible that this file will be called \fname{H10EMP.mi4} instead. If so, rename the \fname{H10.mi4} you downloade in step 1 to \fname{H10EMP.mi4}.}}
+    \opt{h10_5gb}{\note{If you have a Pure model \playertype{} (which doesn't have a FM radio) it is possible that this file will be called \fname{H10EMP.mi4} instead. If so, rename the \fname{H10.mi4} you downloaded in step 1 to \fname{H10EMP.mi4}.}}
     \note{You should keep a safe backup of this file for use if you ever wish to switch back to the \playerman{} firmware.}
-    \note{If you can't see the \fname{System} directory, you will need to make sure your operating system is configured to show hidden files and folers.}
+    \note{If you can't see the \fname{System} directory, you will need to make sure your operating system is configured to show hidden files and folders.}
 
   \item Copy the \opt{h10}{\fname{H10\_20GC.mi4}}\opt{h10_5gb}{\fname{H10.mi4} (or \fname{H10EMP.mi4} if you have a \playertype{} Pure)} file you downloaded to the System directory on your \dap{}.
 \end{enumerate}
-- 
cgit v1.2.3

