From bb1c2ea0b17ed0affe17c647a22ba26bd9f42f8b Mon Sep 17 00:00:00 2001
From: Dana Conrad <dconrad@fastmail.com>
Date: Sun, 15 Sep 2024 15:03:00 -0500
Subject: Fix manual build in 018c54ad1c

Change-Id: If0bce46e161b1f61543c73a4417eda1c179c34a7
---
 manual/getting_started/hibyos_nativeinstall.tex | 14 ++++++--------
 1 file changed, 6 insertions(+), 8 deletions(-)

(limited to 'manual/getting_started/hibyos_nativeinstall.tex')

diff --git a/manual/getting_started/hibyos_nativeinstall.tex b/manual/getting_started/hibyos_nativeinstall.tex
index 9312a8ec71..a5c4f07fed 100644
--- a/manual/getting_started/hibyos_nativeinstall.tex
+++ b/manual/getting_started/hibyos_nativeinstall.tex
@@ -5,13 +5,12 @@ mode. The process is summed up as the following:
   \item Determine what hardware version your player is and download
     the correct bootloader update file
   \item Place the bootloader \fname{update.upt} file on the SD card
-  \item In the original firmware, run the Firmware Update
-    \code{System Settings --> Firmware Update}
+  \item In the original firmware, run the Firmware Update: \\
+    \fname{System Settings --> Firmware Update}
 \end{itemize}
 
 \subsubsection{Determine hardware version}\label{ref:determine_hardware_version}
-Determine what hardware version your player is. Go to
-\code{System Settings --> About The Player --> Version} and reference
+Determine what hardware version your player is. Go to \fname{System Settings --> About The Player --> Version} and reference
 the list below. hw1, hw1.5, and hw2 players all use the same update
 file (with one exception), while hw3 players use a different one.
 
@@ -32,10 +31,9 @@ may not be the most up to date, please see the wiki page at
     \item Hifiwalker H2 V1.1 - V1.6
     \item Surfans F20 V2.2 - V2.7
   \end{itemize}
-
   These players use \fname{erosqnative-hw1hw2-erosq.upt} as the update file.
   The lone exception is the Hifiwalker H2 V1.3, which uses the update file
-  \fname{erosqnative-hw1hw2-eros_h2.upt}.
+  \fname{erosqnative-hw1hw2-eros\_h2.upt}.
 \item[hw3 players]
   \begin{itemize}
     \item Aigo Eros Q V2.1
@@ -61,6 +59,6 @@ Don't forget to safely eject/unmount your player.
 
 \subsubsection{Run Firmware Update}\label{ref:run_firmware_update}
 In the original firmware, run the firmware updater by going to
-\code{System Settings --> Firmware Update}. At this point, you can delete
+\fname{System Settings --> Firmware Update}. At this point, you can delete
 \fname{update.upt} from the SD card if you wish. \emph{Do not delete .rockbox,
-this is your Rockbox installation and needs to stay there!}
\ No newline at end of file
+this is your Rockbox installation and needs to stay there!}
-- 
cgit v1.2.3

