From 018c54ad1c1fdd15759141da11120e00763986cd Mon Sep 17 00:00:00 2001
From: Dana Conrad <dconrad@fastmail.com>
Date: Fri, 13 Sep 2024 12:18:01 -0500
Subject: Manual: Update erosqnative

Update installation instructions, and add a couple things that
were missing.

Change-Id: I7313285338fe5c4bc05a944e3ba2ff941a796d5b
---
 manual/getting_started/installation.tex | 29 +++++++++++++++++++++++++++--
 1 file changed, 27 insertions(+), 2 deletions(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 661964dd8a..04118680b1 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -118,6 +118,15 @@ of before installing.
 \begin{description}
   \item[Filesystem support.] Rockbox only supports the FAT32 filesystem. Other
     filesystems such as exFAT or NTFS are not supported.
+
+    \opt{erosqnative}{\note{Many SD cards come with exFAT on them from the
+    factory. The original firmware can be used to reformat them to FAT
+    by going to \code{System Settings --> Reset --> Format TF Card}.}
+    
+    \note{The SD card that sometimes come bundled with these players are usually
+    of substandard quality and are not to be trusted. It is recommended to source
+    a card of a reputable brand, from a reputable source, such as direct from
+    the manufacturer.}}
   \item[USB DAC.] This feature is not supported by Rockbox, but you can
     dual-boot the original firmware if you want to use it.
   \opt{shanlingq1,agptekrocker,xduoox3ii,xduoox20,aigoerosq,erosqnative}{\item[Wireless.] There is no support for Bluetooth\opt{shanlingq1}{ or WiFi}.
@@ -545,7 +554,8 @@ by Rockbox, in the main directory of your \daps{} drive.
         \opt{samsungyh}{\input{getting_started/samsungyh_install.tex}}
         \opt{xduoox3}{\input{getting_started/xduoox3_install.tex}}
         \opt{xduoox3ii,xduoox20,agptekrocker,aigoerosq}{\input{getting_started/hibyos_install.tex}}
-        \opt{fiiom3k,shanlingq1,erosqnative}{\input{getting_started/jztool_install.tex}}
+        \opt{fiiom3k,shanlingq1}{\input{getting_started/jztool_install.tex}}
+        \opt{erosqnative}{\input{getting_started/hibyos_nativeinstall.tex}}
     }
 }
 
@@ -807,7 +817,7 @@ completely follow the manual uninstallation instructions below.}}
     \playerman{} firmware.
 }
 
-\opt{fiiom3k,shanlingq1,erosqnative}{
+\opt{fiiom3k,shanlingq1}{
     If you want to remove the Rockbox bootloader, copy an original firmware
     update to your microSD card and run the \playerman{} update by 
     \opt{erosqnative}{running it from the Original Firmware's System Settings menu.}
@@ -821,6 +831,21 @@ completely follow the manual uninstallation instructions below.}}
     and enter the recovery menu -- see \reference{ref:jztool_load_bootloader}.
 }
 
+\opt{erosqnative}{
+    If you want to remove the Rockbox bootloader, you will need to acquire the correct
+    update file for your brand player and original firmware version number. The
+    uninstallation procedure can then be done as follows:
+
+    \begin{itemize}
+      \item If the update file is unmodified, use \fname{tools/hibyos_nativepatcher/hibyos_nativepatcher.sh}
+      to mark the original bootloader for updating
+      \item Place the update file on the SD card and ensure it is named \emph{exactly}
+      \fname{update.upt}
+      \item Boot into the Rockbox bootloader menu: With the player off, hold \ButtonVolUp + \ButtonPower
+      \item Select "Aigo Recovery"
+    \end{itemize}
+}
+
 \nopt{gigabeats}{
   If you wish to clean up your disk, you may also wish to delete the
   \fname{.rockbox} directory and its contents.
-- 
cgit v1.2.3

