From 16a0e819859069d0676274c2aa0d1313b4673403 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Wed, 28 Apr 2010 16:02:49 +0000
Subject: Add that you need to be in MSC mode to the fuze manual.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25748 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index ac1d0df1f8..e47ca21da4 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -142,7 +142,7 @@ follow the instructions at
     the USB port through the subpack, not the side 'USB Host' port. The side port
     is intended to be used for USB OTG connections only (digital cameras, memory
     sticks, etc.).
-  }    
+  }
   \opt{sansa,e200v2,clipv1,clipv2,clipplus}{
     \note{The following steps require you to change the setting in
     \setting{Settings $\rightarrow$ USB Mode} to \setting{MSC} from within the
@@ -150,6 +150,13 @@ follow the instructions at
 
     \nopt{sansaAMS}{\warn{Never extract files to your \dap{} while it is in recovery mode.}}
   }
+
+  \opt{fuze}{
+    \note{The following steps require you to change the setting in
+    \setting{Settings $\rightarrow$ System Settings $\rightarrow$ USB Mode} to
+    \setting{MSC} from within the original firmware.}
+  }
+
   \opt{h10,h10_5gb}{
     The installation requires you to use UMS mode and so
     may require use of the UMS trick, whereby it is possible to force a MTP
-- 
cgit v1.2.3

