From 607adf00b5fad553b1b1aeec6b4b16d61b902908 Mon Sep 17 00:00:00 2001
From: Solomon Peachy <pizza@shaftnet.org>
Date: Sun, 15 Sep 2024 15:07:12 -0400
Subject: manual: fix error in 018c54ad1c

Change-Id: I58bc8f726d2c82c0586e982753dda55c028aa3bd
---
 manual/getting_started/installation.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 04118680b1..ff230be203 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -121,8 +121,8 @@ of before installing.
 
     \opt{erosqnative}{\note{Many SD cards come with exFAT on them from the
     factory. The original firmware can be used to reformat them to FAT
-    by going to \code{System Settings --> Reset --> Format TF Card}.}
-    
+    by going to \code{System Settings --> Reset --> Format TF Card}.}}
+
     \note{The SD card that sometimes come bundled with these players are usually
     of substandard quality and are not to be trusted. It is recommended to source
     a card of a reputable brand, from a reputable source, such as direct from
@@ -819,7 +819,7 @@ completely follow the manual uninstallation instructions below.}}
 
 \opt{fiiom3k,shanlingq1}{
     If you want to remove the Rockbox bootloader, copy an original firmware
-    update to your microSD card and run the \playerman{} update by 
+    update to your microSD card and run the \playerman{} update by
     \opt{erosqnative}{running it from the Original Firmware's System Settings menu.}
     \nopt{erosqnative}{holding \ActionBootOFRecovery{} while powering on the \dap{}.}
 
-- 
cgit v1.2.3

