From 6a96037d09c99041bae87ae7c7a5189adafd7408 Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Sun, 9 May 2010 21:03:30 +0000
Subject: Add non-breaking spaces to mA, mAh, MB and GB. Add playertype for
 iPod Video when describing the different variants.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25921 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 16 ++++++++--------
 1 file changed, 8 insertions(+), 8 deletions(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index bc444b3700..02394248e9 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -59,7 +59,7 @@ follow the instructions at
 }
   \opt{cowond2}{
     Rockbox runs on all \playerman{} \playertype{} and \playertype{}+ variants
-    (2 / 4 / 8 / 16GB, with or without DAB/DMB).
+    (2 / 4 / 8 / 16~GB, with or without DAB/DMB).
     \note{Newer \playertype{}+ hardware revisions use an updated power
     management chip, and some functionality is not yet implemented on these
     players (e.g. touchscreen support).}
@@ -317,7 +317,7 @@ filesystem.\\*
 
 \opt{ipodvideo}
     {\note{Autodetection is unable to distinguish between the
-    \playerman{} 30~GB and 60~GB / 80~GB models and defaults to the
+    \playerman{} \playertype{} 30~GB and 60/80~GB models and defaults to the
     30~GB model. This will usually work but you might want to check the
     detected value, especially if you experience problems with Rockbox.}
 }
@@ -411,7 +411,7 @@ straight to \reference{ref:finish_install}
 \subsubsection{Installing the firmware}\label{sec:installing_firmware}
 
 \opt{gigabeats}{\note{When your \dap{} is in the Rockbox USB or bootloader
-USB mode, you will see two visible partitions - the 150MB firmware
+USB mode, you will see two visible partitions - the 150~MB firmware
 partition (containing at least a file called \fname{nk.bin}) and
 the main data partition. Rockbox \emph{must} be installed onto the main
 data partiton.}}
@@ -419,9 +419,9 @@ data partiton.}}
 \begin{enumerate} 
 \item Download your chosen version of Rockbox from the links in the
   previous section.
-\opt{ipodvideo}{\note{There are separate versions of Rockbox for the 30GB and 
-60GB/80GB models.  You must ensure you download the correct version for your 
-\dap{}.}}
+\opt{ipodvideo}{\note{There are separate versions of Rockbox for the 30~GB and 
+60/80~GB \playerman{} \playertype{} models. You must ensure you download the 
+correct version for your \dap{}.}}
 
 \item Connect your \dap{} to the computer via USB 
   \opt{sansa,sansaAMS,h10,h10_5gb,vibe500}{ in MSC mode }
@@ -599,7 +599,7 @@ The new build will be installed over your current build.\\
 
 \opt{gigabeats}{
   \note{When your \dap{} is in the Rockbox USB or bootloader
-  USB mode, you will see two visible partitions, the 150MB firmware
+  USB mode, you will see two visible partitions, the 150~MB firmware
   partition (containing at least a file called \fname{nk.bin}) and
   the main data partition. Rockbox \emph{must} be installed onto the main
   data partiton.\\}
@@ -731,7 +731,7 @@ completely follow the manual uninstallation instructions below.}}
   your favourite unzipping utility e.g. 7zip.
   \item Connect your \dap{} to your computer.
   \item Extract \fname{nk.bin} from within
-  \fname{gbs\_update\_1\_2\_us.exe} using e.g. 7zip and copy it to the 150 MB
+  \fname{gbs\_update\_1\_2\_us.exe} using e.g. 7zip and copy it to the 150~MB
   firmware partition of your \dap{}.
   \item Safely eject / unmount the USB drive, unplug the cable and restart.
   \end{itemize}
-- 
cgit v1.2.3

