From 8867292ee6ceda4419d219835f63655f5e951989 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Wed, 28 Apr 2010 16:16:57 +0000
Subject: Correct path to set MSC mode in the OF for the Clip+

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25749 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index e47ca21da4..b15b63d810 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -143,7 +143,7 @@ follow the instructions at
     is intended to be used for USB OTG connections only (digital cameras, memory
     sticks, etc.).
   }
-  \opt{sansa,e200v2,clipv1,clipv2,clipplus}{
+  \opt{sansa,e200v2,clipv1,clipv2}{
     \note{The following steps require you to change the setting in
     \setting{Settings $\rightarrow$ USB Mode} to \setting{MSC} from within the
     original firmware.}
@@ -151,7 +151,7 @@ follow the instructions at
     \nopt{sansaAMS}{\warn{Never extract files to your \dap{} while it is in recovery mode.}}
   }
 
-  \opt{fuze}{
+  \opt{fuze,clipplus}{
     \note{The following steps require you to change the setting in
     \setting{Settings $\rightarrow$ System Settings $\rightarrow$ USB Mode} to
     \setting{MSC} from within the original firmware.}
-- 
cgit v1.2.3

