From 92ef9b260a5dce9c5ce5e9ffeb34398238b1ace7 Mon Sep 17 00:00:00 2001
From: Michael Giacomelli <giac2000@hotmail.com>
Date: Sun, 8 Jan 2012 07:05:58 +0000
Subject: Clarify that you must reboot into the Sandisk firmware when
 uninstalling the bootloader.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@31630 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 30c8a743ff..559ff0dbce 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -749,7 +749,8 @@ completely follow the manual uninstallation instructions below.}}
 }
 
     \opt{sansaAMS}{
-      Copy an unmodified original firmware to your player and update it.
+      Copy an unmodified original firmware to your player, and then reboot into 
+      the Sandisk firmware.  
 }
 
 \opt{mpiohd200}{
-- 
cgit v1.2.3

