From e0d94f5b586d8323f4f2f82892fc1403fe86f71f Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Fri, 22 Feb 2013 21:10:59 +0000
Subject: Manual: The c200v2 also needs to be set to MSC mode for installation.

Change-Id: If49f35073544fa7b18cbffa6885b4bc4b98c42d4
---
 manual/getting_started/installation.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 2454734a48..146f1d73c4 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -146,7 +146,7 @@ follow the instructions at
     is intended to be used for USB OTG connections only (digital cameras, memory
     sticks, etc.).
   }
-  \opt{sansa,e200v2,clipv1,clipv2,fuzeplus}{
+  \opt{sansa,e200v2,clipv1,clipv2,fuzeplus,c200v2}{
     \note{The following steps require you to change the setting in
     \setting{Settings $\rightarrow$ USB Mode} to \setting{MSC} from within the
     original firmware.}
-- 
cgit v1.2.3

