From b1080ce052b1aa5bc544d8adaec473cb1da309a9 Mon Sep 17 00:00:00 2001
From: Dominik Riebeling <Dominik.Riebeling@gmail.com>
Date: Tue, 6 Jun 2006 19:59:25 +0000
Subject: Fix an arrow. Code policing.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@10078 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/iriver_install.tex | 114 +++++++++++++++---------------
 1 file changed, 57 insertions(+), 57 deletions(-)

(limited to 'manual/getting_started/iriver_install.tex')

diff --git a/manual/getting_started/iriver_install.tex b/manual/getting_started/iriver_install.tex
index 4dcf971047..c92f69a62d 100644
--- a/manual/getting_started/iriver_install.tex
+++ b/manual/getting_started/iriver_install.tex
@@ -1,3 +1,4 @@
+% $Id$ %
 \subsection{Installing the bootloader}
   Installing the bootloader is the trickiest part of the installation.
   The Rockbox bootloader allows users to boot into either the Rockbox 
@@ -8,73 +9,72 @@
   and install it on your jukebox.
 
 \begin{enumerate}
-	\item Download a supported version of the Iriver firmware for your \playername\ from 
-	the Iriver website or from 
-	\url{http://www.rockbox.org/twiki/bin/view/Main/ManualRockboxInstall}.
-	Supported	Iriver firmware versions currently include 
-		\opt{IRIVER_H100_PAD}{1.63US, 1.63EU, 1.63K, 1.65US, 1.65EU, 1.65K, 1.66US, 1.66EU 
-		and 1.66K.  Note that the H140 uses the same firmware as the H120; H120 and H140 owners should use the
-			firmware called \fname{ihp\_120.hex}.  Likewise, the iHP110 and iHP115 use the same 
-			firmware,	called \fname{ihp\_100.hex}.   Be sure to use the correct firmware file
-			for your player.
-		}
-		\opt{IRIVER_H300_PAD}{1.28K, 1.28EU, 1.28J, 1.29K, 1.29J and 1.30EU.\\
-			\note{The US H3xx firmware is not currently supported and cannot be patched to be 
-			used with the bootloader. If you wish to install Rockbox on a US \playername\, you 
-			must use an international firmware, which will permanently remove DRM support from 
-			the player.}
-		}
-		If the file that you downloaded is a \fname{.zip} file, use an unzip 
-		utility such as \fname{InfoZip}, \fname{7zip}, \fname{WinRAR},	or 
-		\fname{WinZip} to extract the \fname{.hex} from the \fname{.zip} file
-		to your desktop. Likewise, if the file that you downloaded is an 
-		\fname{.exe} file, double-click on the \fname{.exe}	file to extract 
-		the \fname{.hex} file to your desktop.
-		
-	\item Download the firmware patcher \fname{fwpatcher.exe} from the site 
-	listed in the prior step and save it to your desktop.
-
- 	\warn{The firmware patcher contains Unicode support, which is not supported by 
-	all versions of Windows. If you have difficulty with the firmware patcher, try 
-	downloading the alternate firmware patcher \fname{fwpatchernu.exe}, which is 
-	built without Unicode support.}
-
+  \item Download a supported version of the Iriver firmware for your 
+  \playername\ from the Iriver website or from 
+  \wikilink{ManualRockboxInstall}.
+  Supported Iriver firmware versions currently include 
+  \opt{IRIVER_H100_PAD}{1.63US, 1.63EU, 1.63K, 1.65US, 1.65EU, 1.65K, 1.66US, 
+    1.66EU and 1.66K.  Note that the H140 uses the same firmware as the H120;
+    H120 and H140 owners should use the	firmware called \fname{ihp\_120.hex}.
+    Likewise, the iHP110 and iHP115 use the same firmware, called 
+    \fname{ihp\_100.hex}.   Be sure to use the correct firmware file for 
+    your player.}
+  \opt{IRIVER_H300_PAD}{1.28K, 1.28EU, 1.28J, 1.29K, 1.29J and 1.30EU.
+    \note{The US H3xx firmware is not currently supported and cannot be
+    patched to be used with the bootloader. If you wish to install Rockbox
+    on a US \playername\, you must use an international firmware, which will
+    permanently remove DRM support from the player.}
+  }
+  If the file that you downloaded is a \fname{.zip} file, use an unzip 
+  utility such as \fname{InfoZip}, \fname{7zip}, \fname{WinRAR},	or 
+  \fname{WinZip} to extract the \fname{.hex} from the \fname{.zip} file
+  to your desktop. Likewise, if the file that you downloaded is an 
+  \fname{.exe} file, double-click on the \fname{.exe}	file to extract 
+  the \fname{.hex} file to your desktop.
+  %
+  \item Download the firmware patcher \fname{fwpatcher.exe} from the site 
+  listed in the prior step and save it to your desktop.
+    \warn{The firmware patcher contains Unicode support, which is not supported by 
+    all versions of Windows. If you have difficulty with the firmware patcher, try 
+    downloading the alternate firmware patcher \fname{fwpatchernu.exe}, which is 
+    built without Unicode support.}
+  %
   \item Go to your desktop and double-click on whichever version of the firmware 
   patcher you downloaded in the prior step.
-  
+  %
   \item In the firmware patcher dialog box, click on the BROWSE button and navigate
   to the \fname{.hex} file that you previously downloaded to your desktop.
-  	
+  %
   \item Click PATCH. The firmware patcher will patch the original firmware to 
   include the Rockbox bootloader. The \fname{.hex} file on your desktop is now
   a modified version of the original \fname{.hex} file.
-  
+  %
   \item Turn on your \playername\ and connect it to your computer via USB.
-  
-	\item Copy or move the modified \fname{.hex} file to the ROOT directory of 
-	your jukebox.
-
+  %
+  \item Copy or move the modified \fname{.hex} file to the ROOT directory of 
+    your jukebox.
+  %
   \item Disconnect the jukebox from USB. (Be sure to use Windows' ``safely remove
   hardware'' option.)
+  \warn{Before proceeding further, make sure that your player has a full charge, 
+    or that it is connected to the power adaptor.}
+  %
+  \item Update your \playername s firmware with the patched bootloader. To do this, turn 
+    the jukebox on. Press and hold the 
+    \opt{IRIVER_H100_PAD}{\ButtonSelect{} button }
+    \opt{IRIVER_H300_PAD}{\ButtonSelect{} button }
+    to enter the main menu, and navigate to \setting{General $\rightarrow$ Firmware 
+    Upgrade}. Select \setting{Yes} when asked to confirm if you want to upgrade the 
+    firmware. The \playername{} will display a message indicating that the
+    firmware update 
+    is in progress. Do not interrupt this process. When the firmware update is 
+    complete, the player will turn itself off. (The update firmware process usually 
+    takes a minute or so.)
 
-	\warn{Before proceeding further, make sure that your player has a full charge, 
-	or that it is connected to the power adaptor.}
-
-	\item Update your \playername s firmware with the patched bootloader. To do this, turn 
-	the jukebox on. Press and hold the 
-	\opt{IRIVER_H100_PAD}{\ButtonSelect\ button }
-	\opt{IRIVER_H300_PAD}{\ButtonSelect button }
-	 to enter the main menu, and navigate to \setting{General} --> \setting{Firmware 
-	 Upgrade}. Select \setting{Yes} when asked to confirm if you want to upgrade the 
-	 firmware. The \playername\ will display a message indicating that the firmware update 
-	 is in progress. Do not interrupt this process. When the firmware update is 
-	 complete, the player will turn itself off. (The update firmware process usually 
-	 takes a minute or so.)
-
-You have now installed the Rockbox bootloader. 
+    You have now installed the Rockbox bootloader. 
 
-\opt{H1xx}{\note{If you install the Rockbox bootloader, but do not install the
-Rockbox firmware, the Rockbox bootloader will load the iriver firmware when the
-jukebox is turned on.}}
+\opt{h1xx}{\note{If you install the Rockbox bootloader, but do not install the
+  Rockbox firmware, the Rockbox bootloader will load the iriver firmware when the
+  jukebox is turned on.}}
 
-\end{enumerate}
\ No newline at end of file
+\end{enumerate}
-- 
cgit v1.2.3

