From f8e2f3e08d779092cf7d3f26f369c0941edf9349 Mon Sep 17 00:00:00 2001
From: Martin Arver <martin.arver@gmail.com>
Date: Tue, 17 Oct 2006 12:18:51 +0000
Subject: Fix for more consistent and proper British English. (-ize/-ise etc)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@11246 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/iriver_install.tex | 40 +++++++++++++++----------------
 1 file changed, 20 insertions(+), 20 deletions(-)

(limited to 'manual/getting_started/iriver_install.tex')

diff --git a/manual/getting_started/iriver_install.tex b/manual/getting_started/iriver_install.tex
index fb950a23dd..0cb59492e8 100644
--- a/manual/getting_started/iriver_install.tex
+++ b/manual/getting_started/iriver_install.tex
@@ -1,11 +1,11 @@
 % $Id$ %
 
-  Installing the bootloader is the trickiest part of the installation.
-  The Rockbox bootloader allows users to boot into either the Rockbox 
-  firmware or the iriver firmware. For legal reasons, we cannot distribute 
-  the bootloader. Instead, we have developed a program that will patch the 
-  Iriver firmware with the Rockbox bootloader. These instructions will explain 
-  how to download and patch the Iriver firmware with the Rockbox bootloader 
+  Installing the boot loader is the trickiest part of the installation.
+  The Rockbox boot loader allows users to boot into either the Rockbox 
+  firmware or the \playerman{} firmware. For legal reasons, we cannot distribute 
+  the boot loader. Instead, we have developed a program that will patch the 
+  Iriver firmware with the Rockbox boot loader. These instructions will explain 
+  how to download and patch the Iriver firmware with the Rockbox boot loader 
   and install it on your jukebox.
 
 
@@ -22,7 +22,7 @@
     your player.}
   \opt{IRIVER_H300_PAD}{1.28K, 1.28EU, 1.28J, 1.29K, 1.29J and 1.30EU.
     \note{The US H3xx firmware is not currently supported and cannot be
-    patched to be used with the bootloader. If you wish to install Rockbox
+    patched to be used with the boot loader. If you wish to install Rockbox
     on a US \playername, you must use an international firmware, which will
     permanently remove DRM support from the player.}
   }%
@@ -32,7 +32,7 @@
   to your desktop. Likewise, if the file that you downloaded is an 
   \fname{.exe} file, double-click on the \fname{.exe} file to extract 
   the \fname{.hex} file to your desktop.
-  When running linux you should be able extracting \fname{.exe}
+  When running Linux you should be able extracting \fname{.exe}
   files using \fname{unzip}.
   %
   \item Download the firmware patcher \fname{fwpatcher.exe} from 
@@ -50,7 +50,7 @@
   to the \fname{.hex} file that you previously downloaded to your desktop.
   %
   \item Click \setting{Patch}. The firmware patcher will patch the
-    original firmware to include the Rockbox bootloader. The \fname{.hex}
+    original firmware to include the Rockbox boot loader. The \fname{.hex}
     file on your desktop is now a modified version of the original
     \fname{.hex} file.
   %
@@ -65,7 +65,7 @@
     or that it is connected to the power adaptor. Interrupting the next step
     due to a power failure most likely will brick your \dap{}.}
   %
-  \item Update your \daps{} firmware with the patched bootloader. To do this, turn
+  \item Update your \daps{} firmware with the patched boot loader. To do this, turn
     the jukebox on. Press and hold the
     \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonSelect{} button }%
     to enter the main menu, and navigate to \setting{General $\rightarrow$ Firmware 
@@ -76,24 +76,24 @@
     firmware update is complete the player will turn itself off. (The update
     firmware process usually takes a minute or so.)
     
-    You have now installed the Rockbox bootloader.
+    You have now installed the Rockbox boot loader.
 \end{enumerate}
 
-\note{If you install the Rockbox bootloader but do not install the
-  Rockbox firmware the Rockbox bootloader will load the iriver firmware when the
+\note{If you install the Rockbox boot loader but do not install the
+  Rockbox firmware the Rockbox boot loader will load the Iriver firmware when the
   jukebox is turned on.
   To load the \playerman{} firmware press and hold \ButtonRec{} before
   powering up the \dap{} until the \playerman{} logo appears.
   }
 
-\note{The bootloader has a builtin ``bootloader USB mode''. This function
+\note{The boot loader has a built-in ``boot loader USB mode''. This function
   switches to USB mode when the \dap{} is connected to a computer upon
-  power-up. This way you can access the \daps{} harddisk without the need
-  to boot any firmware (which is also useful when your harddisk is 
-  damaged). The screen will simply display the text ``bootloader USB mode''.
-  After you disconnect the \dap{} from USB the bootloader will
-  continue booting Rockbox. As in bootloader USB mode the firmware
+  power-up. This way you can access the \daps{} hard disk without the need
+  to boot any firmware (which is also useful when your hard disk is 
+  damaged). The screen will simply display the text ``boot loader USB mode''.
+  After you disconnect the \dap{} from USB the boot loader will
+  continue booting Rockbox. As in boot loader USB mode the firmware
   itself hasn't been loaded this is also a simple way of updating Rockbox.
-  After the disconnect the bootloader will load the updated version of
+  After the disconnect the boot loader will load the updated version of
   Rockbox.
 }
-- 
cgit v1.2.3

