From 2b0db13b51c545dca3988489bddb7b03c03afaf5 Mon Sep 17 00:00:00 2001
From: Rafaël Carré <rafael.carre@gmail.com>
Date: Wed, 25 Aug 2010 13:45:03 +0000
Subject: Manual: fix Sansa AMS install

Sandisk has changed its forum, so update the links to OF
Also add c200v2 link and description

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@27879 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/sansaAMS_install.tex | 19 +++++++++++++------
 1 file changed, 13 insertions(+), 6 deletions(-)

(limited to 'manual/getting_started/sansaAMS_install.tex')

diff --git a/manual/getting_started/sansaAMS_install.tex b/manual/getting_started/sansaAMS_install.tex
index 3f3fbd97c5..8a977f885d 100644
--- a/manual/getting_started/sansaAMS_install.tex
+++ b/manual/getting_started/sansaAMS_install.tex
@@ -6,13 +6,15 @@ files:
 \begin{itemize}
   \item An original firmware (OF) from 
     \opt{e200v2}{
-      \url{http://forums.sandisk.com/sansa/board/message?board.id=e200&thread.id=13548}}
+      \url{http://forums.sandisk.com/t5/User-guides-Firmware-Software/e200v2-03-01-16-Firmware-Download-amp-Instructions/td-p/36562}}
     \opt{fuze,fuzev2}{
-      \url{http://forums.sandisk.com/sansa/board/message?board.id=sansafuse&thread.id=23276}}
+      \url{http://forums.sandisk.com/t5/Fuze/Sansa-Fuze-Firmware-Update-01-02-31-amp-02-03-33/td-p/139175}}
     \opt{clipv1,clipv2}{
-      \url{http://forums.sandisk.com/sansa/board/message?board.id=clip&thread.id=15109}}
+      \url{http://forums.sandisk.com/t5/Clip-Clip/Sansa-Clip-Firmware-01-01-35-amp-02-01-35-Release/td-p/144965}}
     \opt{clipplus}{
-      \url{http://forums.sandisk.com/sansa/board/message?board.id=clipplus&thread.id=2911}}
+      \url{http://forums.sandisk.com/t5/Clip-Clip/Sansa-Clip-Firmware-Update-01-02-15/td-p/150227}}
+    \opt{c200v2}{
+      \url{http://forums.sandisk.com/t5/User-guides-Firmware-Software/c200-version2-Latest-Firmware-Installation-Instructions-03-02-05/td-p/34097}}
 
   \item The bootloader: 
     \opt{e200v2}{\download{bootloader/sandisk-sansa/e200v2/bootloader-e200v2.sansa}}
@@ -21,6 +23,7 @@ files:
     \opt{clipv1}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}
     \opt{clipv2}{\download{bootloader/sandisk-sansa/clipv2/bootloader-clipv2.sansa}}
     \opt{clipplus}{\download{bootloader/sandisk-sansa/clipplus/bootloader-clipplus.sansa}}
+    \opt{c200v2}{\download{bootloader/sandisk-sansa/c200v2/bootloader-c200v2.sansa}}
 
   \item The version of mkamsboot for your operating system from
     \download{bootloader/sandisk-sansa/mkamsboot/}
@@ -45,6 +48,7 @@ files:
     \opt{clipv1}{mkamsboot.exe m300a.bin bootloader-clip.sansa patched.bin}
     \opt{clipv2}{mkamsboot.exe m30pa.bin bootloader-clipv2.sansa patched.bin}
     \opt{clipplus}{mkamsboot.exe clppa.bin bootloader-clipplus.sansa patched.bin}
+    \opt{c200v2}{mkamsboot.exe c200pa.bin bootloader-c200v2.sansa patched.bin}
   \end{code}
  
   If mkamsboot.exe does not report success, then retry or abort.
@@ -53,7 +57,8 @@ files:
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
-  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''} above).
+  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''}
+  \opt{c200v2}{(``c200pa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
@@ -77,6 +82,7 @@ files:
     \opt{clipv1}{./mkamsboot m300a.bin bootloader-clip.sansa patched.bin}
     \opt{clipv2}{./mkamsboot m30pa.bin bootloader-clipv2.sansa patched.bin}
     \opt{clipplus}{./mkamsboot clppa.bin bootloader-clipplus.sansa patched.bin}
+    \opt{c200v2}{./mkamsboot c200pa.bin bootloader-c200v2.sansa patched.bin}
   \end{code}
  
   If mkamsboot does not report success, then retry or abort.
@@ -85,7 +91,8 @@ files:
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
-  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''} above).
+  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''}
+  \opt{c200v2}{(``c200pa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
-- 
cgit v1.2.3

