From 4c6b94551e5e8eef36f6919d3992dc9f331562c1 Mon Sep 17 00:00:00 2001
From: Rafaël Carré <rafael.carre@gmail.com>
Date: Thu, 20 May 2010 18:34:05 +0000
Subject: fuzev2: make manual build

Use the same info than Clipv1/v2 to warn about the version
(the path in OF menu to check the version has just one more component on Fuze)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@26205 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/sansaAMS_install.tex | 9 ++++++---
 1 file changed, 6 insertions(+), 3 deletions(-)

(limited to 'manual/getting_started/sansaAMS_install.tex')

diff --git a/manual/getting_started/sansaAMS_install.tex b/manual/getting_started/sansaAMS_install.tex
index 44bfa2c64b..3f3fbd97c5 100644
--- a/manual/getting_started/sansaAMS_install.tex
+++ b/manual/getting_started/sansaAMS_install.tex
@@ -7,7 +7,7 @@ files:
   \item An original firmware (OF) from 
     \opt{e200v2}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=e200&thread.id=13548}}
-    \opt{fuze}{
+    \opt{fuze,fuzev2}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=sansafuse&thread.id=23276}}
     \opt{clipv1,clipv2}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=clip&thread.id=15109}}
@@ -17,6 +17,7 @@ files:
   \item The bootloader: 
     \opt{e200v2}{\download{bootloader/sandisk-sansa/e200v2/bootloader-e200v2.sansa}}
     \opt{fuze}{\download{bootloader/sandisk-sansa/fuze/bootloader-fuze.sansa}}
+    \opt{fuzev2}{\download{bootloader/sandisk-sansa/fuzev2/bootloader-fuzev2.sansa}}
     \opt{clipv1}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}
     \opt{clipv2}{\download{bootloader/sandisk-sansa/clipv2/bootloader-clipv2.sansa}}
     \opt{clipplus}{\download{bootloader/sandisk-sansa/clipplus/bootloader-clipplus.sansa}}
@@ -39,6 +40,7 @@ files:
 
   \begin{code} 
     \opt{fuze}{mkamsboot.exe fuzea.bin bootloader-fuze.sansa patched.bin}
+    \opt{fuzev2}{mkamsboot.exe fuzpa.bin bootloader-fuzev2.sansa patched.bin}
     \opt{e200v2}{mkamsboot.exe e200pe.bin bootloader-e200v2.sansa patched.bin}
     \opt{clipv1}{mkamsboot.exe m300a.bin bootloader-clip.sansa patched.bin}
     \opt{clipv2}{mkamsboot.exe m30pa.bin bootloader-clipv2.sansa patched.bin}
@@ -51,7 +53,7 @@ files:
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
-  \opt{clipplus}{(``clppa.bin''} above).
+  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
@@ -70,6 +72,7 @@ files:
 
   \begin{code} 
     \opt{fuze}{./mkamsboot fuzea.bin bootloader-fuze.sansa patched.bin}
+    \opt{fuzev2}{./mkamsboot fuzpa.bin bootloader-fuzev2.sansa patched.bin}
     \opt{e200v2}{./mkamsboot e200pe.bin bootloader-e200v2.sansa patched.bin}
     \opt{clipv1}{./mkamsboot m300a.bin bootloader-clip.sansa patched.bin}
     \opt{clipv2}{./mkamsboot m30pa.bin bootloader-clipv2.sansa patched.bin}
@@ -82,7 +85,7 @@ files:
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
-  \opt{clipplus}{(``clppa.bin''} above).
+  \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
-- 
cgit v1.2.3

