From 9eb9d30fff16baaf22ffca66ac73c4e85593dd44 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Sat, 21 Nov 2009 17:58:07 +0000
Subject: Update Sansa Clip install instructions in the manual.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@23682 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/sansaAMS_install.tex | 11 +++++++++--
 1 file changed, 9 insertions(+), 2 deletions(-)

(limited to 'manual/getting_started/sansaAMS_install.tex')

diff --git a/manual/getting_started/sansaAMS_install.tex b/manual/getting_started/sansaAMS_install.tex
index 06ef577c44..7ef2eedf17 100644
--- a/manual/getting_started/sansaAMS_install.tex
+++ b/manual/getting_started/sansaAMS_install.tex
@@ -9,10 +9,13 @@ files:
       \url{http://forums.sandisk.com/sansa/board/message?board.id=e200&thread.id=13548}}
     \opt{fuze}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=sansafuse&thread.id=23276}}
+    \opt{clip}{
+      \url{http://forums.sandisk.com/sansa/board/message?board.id=clip&thread.id=15109}}
 
   \item The bootloader: 
     \opt{e200v2}{\download{bootloader/sandisk-sansa/e200v2/bootloader-e200v2.sansa}}
     \opt{fuze}{\download{bootloader/sandisk-sansa/fuze/bootloader-fuze.sansa}}
+    \opt{clip}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}
 
   \item The version of mkamsboot for your operating system from
     \download{bootloader/sandisk-sansa/mkamsboot/}
@@ -33,13 +36,15 @@ files:
   \begin{code} 
     \opt{fuze}{mkamsboot.exe fuzea.bin bootloader-fuze.sansa patched.bin}
     \opt{e200v2}{mkamsboot.exe e200pe.bin bootloader-e200v2.sansa patched.bin}
+    \opt{clip}{mkamsboot.exe m300a.bin bootloader-clip.sansa patched.bin}
   \end{code}
  
   If mkamsboot.exe does not report success, then retry or abort.
 
 \item Copy the output file (``patched.bin'' in the example given above) to the
   root of the device and rename it to the same name as the OF file you downloaded earlier 
-  \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''} above).
+  \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
+  \opt{clip}{(``m300a.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
@@ -59,13 +64,15 @@ files:
   \begin{code} 
     \opt{fuze}{./mkamsboot fuzea.bin bootloader-fuze.sansa patched.bin}
     \opt{e200v2}{./mkamsboot e200pe.bin bootloader-e200v2.sansa patched.bin}
+    \opt{clip}{./mkamsboot m300a.bin bootloader-clip.sansa patched.bin}
   \end{code}
  
   If mkamsboot does not report success, then retry or abort.
 
 \item Copy the output file (``patched.bin'' in the example given above) to the
   root of the device and rename it to the same name as the OF file you downloaded earlier 
-  \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''} above).
+  \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
+  \opt{clip}{(``m300a.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
-- 
cgit v1.2.3

