From cd99b0dbf98bc89c762387d6f4e2da35e181d24f Mon Sep 17 00:00:00 2001
From: Michael Giacomelli <giac2000@hotmail.com>
Date: Sat, 14 Jan 2012 16:32:33 -0500
Subject: Fix install directions for the Clip Zip.

Change-Id: I66214cd44afda7cba18f94f52d7979bcd9e8edd1
---
 manual/getting_started/sansaAMS_install.tex | 23 ++++++++++++++++-------
 1 file changed, 16 insertions(+), 7 deletions(-)
 mode change 100644 => 100755 manual/getting_started/sansaAMS_install.tex

(limited to 'manual/getting_started/sansaAMS_install.tex')

diff --git a/manual/getting_started/sansaAMS_install.tex b/manual/getting_started/sansaAMS_install.tex
old mode 100644
new mode 100755
index 7ceb7d3d30..537cedd0c0
--- a/manual/getting_started/sansaAMS_install.tex
+++ b/manual/getting_started/sansaAMS_install.tex
@@ -15,6 +15,8 @@ files:
       \url{http://forums.sandisk.com/t5/Clip-Clip/Sansa-Clip-Firmware-Update-01-02-15/td-p/150227}}%
     \opt{c200v2}{
       \url{http://forums.sandisk.com/t5/User-guides-Firmware-Software/c200-version2-Latest-Firmware-Installation-Instructions-03-02-05/td-p/34097}}
+    \opt{clipzip}{
+      \url{http://forums.sandisk.com/t5/Clip-Zip/Sansa-Clip-Zip-Firmware-01-01-18/td-p/254122}}
 
   \item The bootloader:
     \opt{e200v2}{\download{bootloader/sandisk-sansa/e200v2/bootloader-e200v2.sansa}}%
@@ -23,7 +25,8 @@ files:
     \opt{clipv1}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}%
     \opt{clipv2}{\download{bootloader/sandisk-sansa/clipv2/bootloader-clipv2.sansa}}%
     \opt{clipplus}{\download{bootloader/sandisk-sansa/clipplus/bootloader-clipplus.sansa}}%
-    \opt{c200v2}{\download{bootloader/sandisk-sansa/c200v2/bootloader-c200v2.sansa}}
+    \opt{c200v2}{\download{bootloader/sandisk-sansa/c200v2/bootloader-c200v2.sansa}}%
+    \opt{clipzip}{\download{bootloader/sandisk-sansa/clipzip/bootloader-clipzip.sansa}}
 
   \item The version of mkamsboot for your operating system from
     \download{bootloader/sandisk-sansa/mkamsboot/}
@@ -45,9 +48,11 @@ files:
   % of the code block. This is necessary as using \opt{} in the code block would
   % create unwanted empty lines.
   \begin{code}[firstline=\opt{fuze}{1}\opt{fuzev2}{2}\opt{e200v2}{3}%
-            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7},%
+            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}%
+            \opt{clipzip}{8},%
                lastline=\opt{fuze}{1}\opt{fuzev2}{2}\opt{e200v2}{3}%
-            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}]
+            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}%
+            \opt{clipzip}{8}]
     mkamsboot.exe fuzea.bin bootloader-fuze.sansa patched.bin
     mkamsboot.exe fuzpa.bin bootloader-fuzev2.sansa patched.bin
     mkamsboot.exe e200pe.bin bootloader-e200v2.sansa patched.bin
@@ -55,6 +60,7 @@ files:
     mkamsboot.exe m30pa.bin bootloader-clipv2.sansa patched.bin
     mkamsboot.exe clppa.bin bootloader-clipplus.sansa patched.bin
     mkamsboot.exe c200pa.bin bootloader-c200v2.sansa patched.bin
+    mkamsboot.exe clpza.bin bootloader-clipzip.sansa patched.bin
   \end{code}
  
   If mkamsboot.exe does not report success, then retry or abort.
@@ -64,7 +70,7 @@ files:
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
   \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''}
-  \opt{c200v2}{(``c200pa.bin''} above).
+  \opt{clipzip}{(``clpza.bin''} \opt{c200v2}{(``c200pa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
@@ -83,9 +89,11 @@ files:
 
 % See above for the code environment arguments explanation.
   \begin{code}[firstline=\opt{fuze}{1}\opt{fuzev2}{2}\opt{e200v2}{3}%
-            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7},%
+            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}%
+            \opt{clipzip}{8},%
                lastline=\opt{fuze}{1}\opt{fuzev2}{2}\opt{e200v2}{3}%
-            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}]
+            \opt{clipv1}{4}\opt{clipv2}{5}\opt{clipplus}{6}\opt{c200v2}{7}%
+            \opt{clipzip}{8}]
     ./mkamsboot fuzea.bin bootloader-fuze.sansa patched.bin
     ./mkamsboot fuzpa.bin bootloader-fuzev2.sansa patched.bin
     ./mkamsboot e200pe.bin bootloader-e200v2.sansa patched.bin
@@ -93,6 +101,7 @@ files:
     ./mkamsboot m30pa.bin bootloader-clipv2.sansa patched.bin
     ./mkamsboot clppa.bin bootloader-clipplus.sansa patched.bin
     ./mkamsboot c200pa.bin bootloader-c200v2.sansa patched.bin
+    ./mkamsboot clpza.bin bootloader-clipzip.sansa patched.bin
   \end{code}
  
   If mkamsboot does not report success, then retry or abort.
@@ -102,7 +111,7 @@ files:
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
   \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
   \opt{clipplus}{(``clppa.bin''} \opt{fuzev2}{(``fuzpa.bin''}
-  \opt{c200v2}{(``c200pa.bin''} above).
+  \opt{c200v2}{(``c200pa.bin''} \opt{clipzip}{(``clpza.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
-- 
cgit v1.2.3

