From 4c745fe8ac2a74262fbea038f7056e2f376734f0 Mon Sep 17 00:00:00 2001
From: Solomon Peachy <pizza@shaftnet.org>
Date: Sun, 22 Aug 2021 07:51:37 -0400
Subject: xduoox3: A few manual improvements

 * Fix a typo in a URL
 * Note how to enter the OF from the bootloader
 * Document how to perform a hard reset

Change-Id: I96d0d64cbd251573e1c5c55657ee5c5db510d9a6
---
 manual/getting_started/xduoox3_install.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/getting_started/xduoox3_install.tex')

diff --git a/manual/getting_started/xduoox3_install.tex b/manual/getting_started/xduoox3_install.tex
index 1a1e05d62e..8390bc6ce7 100644
--- a/manual/getting_started/xduoox3_install.tex
+++ b/manual/getting_started/xduoox3_install.tex
@@ -8,7 +8,7 @@
   \download{bootloader/xduoo/X3-v11.bsdiff}
 
 \item Get a copy of the original \playertype{} v1.1 firmware from
-  \url{httpss://www.xduoo.net/firmware-download/} and extract the .rar file to obtain the
+  \url{https://www.xduoo.net/firmware-download/} and extract the .rar file to obtain the
   update image (called \fname{update.zip}).
 
 \item Compile bspatch in rbutil/bspatch/ (run make in the dir).
@@ -20,7 +20,7 @@
 
 \item Put \fname{output.zip} in the root of the SD card and rename it to \fname{update.zip}.
 
-\item Disconnect the player from USB and let the original firmware boot.
+\item Disconnect the player from USB and let the original firmware boot. If you have already installed the rockbox bootloader you will need to engage the hold/lock switch to force booting into the original firmware.
 
 \item Go into the 'Setting' menu, and select 'Upgrade'. The player will reboot into Rockbox
   upon completion.
-- 
cgit v1.2.3

