From b7b0c7c648f5bf628ebc645e3fd1737b1647eb54 Mon Sep 17 00:00:00 2001
From: Solomon Peachy <pizza@shaftnet.org>
Date: Thu, 19 Nov 2020 09:51:23 -0500
Subject: languages:  convert recording_swcodec -> recording

Change-Id: I481a53284d63457717f4a6524edc5b477f29a20a
---
 manual/main_menu/recording_screen.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/main_menu/recording_screen.tex')

diff --git a/manual/main_menu/recording_screen.tex b/manual/main_menu/recording_screen.tex
index 0d1de44c83..eda5270243 100644
--- a/manual/main_menu/recording_screen.tex
+++ b/manual/main_menu/recording_screen.tex
@@ -16,13 +16,13 @@ front of the peak meters shows the number of times the clip indicator was
 activated during recording. The counter is reset to zero when starting a new
 recording.\\*
 
-\opt{recording_swcodec}{
+\opt{recording}{
 \opt{disk_storage}{
 \note{When you start a recording, the hard disk will spin up. This will cause
 the peak meters to freeze in the process. This is expected behaviour, and
 nothing to worry about. The recording continues during the spin up.\\*}}}
 
-\opt{recording_swcodec}{The frequency and channels} settings are shown in the
+\opt{recording}{The frequency and channels} settings are shown in the
 status bar.\\*
 
 The controls for this screen are:
-- 
cgit v1.2.3

