From d6eefbb21959f690d2da703a7ca421ac5be9c5fa Mon Sep 17 00:00:00 2001
From: Franklin Wei <git@fwei.tk>
Date: Mon, 17 Apr 2017 17:30:42 -0400
Subject: manual: typo fixes

Change-Id: I4a86e031c2dccd2a60b6d0d3fd7cca5df1d88774
---
 manual/plugins/alpinecdc.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/plugins/alpinecdc.tex')

diff --git a/manual/plugins/alpinecdc.tex b/manual/plugins/alpinecdc.tex
index 8d0fcee746..09e5a81b89 100644
--- a/manual/plugins/alpinecdc.tex
+++ b/manual/plugins/alpinecdc.tex
@@ -30,7 +30,7 @@ ASCII art of the 4-pin headphone plug:
 
 The remote pin can be programmed bidirectional, that is the reason this works.
 Very luckily the M-Bus uses a single wire communication and the two radios I
-tried are happy with the 3.3 Volt level the Arcos can deliver. So the
+tried are happy with the 3.3 Volt level the Archos can deliver. So the
 connection is a simple cable! For all protocols requiring more lines, an
 external controller would be necessary.
 
-- 
cgit v1.2.3

