From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/brickmania.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/plugins/brickmania.tex')

diff --git a/manual/plugins/brickmania.tex b/manual/plugins/brickmania.tex
index 2f693eaf81..8065a5cbd4 100644
--- a/manual/plugins/brickmania.tex
+++ b/manual/plugins/brickmania.tex
@@ -56,7 +56,7 @@ effect, you must catch it with the paddle. Look out for the bad ones.\\
     \opt{GIGABEAT_S_PAD}{\ButtonBack}
     \opt{PBELL_VIBE500_PAD}{\ButtonRec}
     \opt{MPIO_HD300_PAD}{\ButtonMenu}
-    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonFF}
+    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
        \opt{HAVEREMOTEKEYMAP}{& 
           \opt{IRIVER_RC_H100_PAD}{\ButtonRCStop}
           }
-- 
cgit v1.2.3

