From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/flipit.tex | 15 ++++++++-------
 1 file changed, 8 insertions(+), 7 deletions(-)

(limited to 'manual/plugins/flipit.tex')

diff --git a/manual/plugins/flipit.tex b/manual/plugins/flipit.tex
index 4d6331750a..8aa8a293ba 100644
--- a/manual/plugins/flipit.tex
+++ b/manual/plugins/flipit.tex
@@ -17,13 +17,13 @@ a screen containing tokens of only one colour.
        \opt{HAVEREMOTEKEYMAP}{& }
 \opt{COWON_D2_PAD}{\TouchTopMiddle{} / \TouchBottomMiddle{} / \TouchMidLeft{} / \TouchMidRight}
     & Move the cursor \\
-\opt{PLAYER_PAD,RECORDER_PAD}{\ButtonPlay}
+\opt{PLAYER_PAD,RECORDER_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonPlay}
 \opt{ONDIO_PAD}{\ButtonMenu}
 \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IPOD_4G_PAD,IPOD_3G_PAD,IAUDIO_X5_PAD%
     ,SANSA_E200_PAD,SANSA_FUZE_PAD,SANSA_C200_PAD,GIGABEAT_PAD,GIGABEAT_S_PAD%
     ,MROBE100_PAD,SANSA_FUZEPLUS_PAD}
     {\ButtonSelect}
-\opt{IRIVER_H10_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
+\opt{IRIVER_H10_PAD}{\ButtonRew}
 \opt{COWON_D2_PAD}{\TouchCenter}
 \opt{PBELL_VIBE500_PAD}{\ButtonOK}
 \opt{MPIO_HD300_PAD}{\ButtonEnter}
@@ -41,8 +41,8 @@ a screen containing tokens of only one colour.
 \opt{SANSA_FUZE_PAD}{\ButtonSelect+\ButtonLeft}
 \opt{GIGABEAT_PAD,GIGABEAT_S_PAD,MROBE100_PAD}{\ButtonMenu}
 \opt{COWON_D2_PAD}{\TouchTopRight}
-\opt{PBELL_VIBE500_PAD,MPIO_HD300_PAD,SANSA_FUZEPLUS_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}%
-    {\ButtonPlay}
+\opt{PBELL_VIBE500_PAD,MPIO_HD300_PAD,SANSA_FUZEPLUS_PAD}{\ButtonPlay}
+\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
        \opt{HAVEREMOTEKEYMAP}{& }
     & Shuffle \\
 \opt{PLAYER_PAD}{\ButtonOn+\ButtonRight}
@@ -59,7 +59,7 @@ a screen containing tokens of only one colour.
 \opt{COWON_D2_PAD}{\TouchBottomLeft}
 \opt{PBELL_VIBE500_PAD,MPIO_HD300_PAD}{\ButtonMenu}
 \opt{SANSA_FUZEPLUS_PAD}{\ButtonBack}
-\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonFF}
+\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{Long \ButtonFF}
        \opt{HAVEREMOTEKEYMAP}{& }
     & Solve \\
 \opt{PLAYER_PAD}{\ButtonOn+\ButtonPlay}
@@ -78,7 +78,7 @@ a screen containing tokens of only one colour.
 \opt{PBELL_VIBE500_PAD}{\ButtonCancel}
 \opt{MPIO_HD300_PAD}{\ButtonRec}
 \opt{SANSA_FUZEPLUS_PAD}{\ButtonBottomLeft}
-\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonFF+\ButtonUp}
+\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonFF}
        \opt{HAVEREMOTEKEYMAP}{& }
     & Solve step by step \\
 \opt{PLAYER_PAD}{\ButtonStop}
@@ -88,7 +88,8 @@ a screen containing tokens of only one colour.
     ,SANSA_C200_PAD,SANSA_CLIP_PAD,COWON_D2_PAD,SANSA_FUZEPLUS_PAD}{\ButtonPower}
 \opt{SANSA_FUZE_PAD}{Long \ButtonHome}
 \opt{GIGABEAT_S_PAD}{\ButtonBack}
-\opt{PBELL_VIBE500_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRec}
+\opt{PBELL_VIBE500_PAD}{\ButtonRec}
+\opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{Long \ButtonRew}
 \opt{MPIO_HD300_PAD}{Long \ButtonMenu}
        \opt{HAVEREMOTEKEYMAP}{& 
           \opt{IRIVER_RC_H100_PAD}{\ButtonRCStop}
-- 
cgit v1.2.3

