From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/metronome.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/plugins/metronome.tex')

diff --git a/manual/plugins/metronome.tex b/manual/plugins/metronome.tex
index 760507e9b9..fca34eb91f 100644
--- a/manual/plugins/metronome.tex
+++ b/manual/plugins/metronome.tex
@@ -46,7 +46,7 @@ on the appropriate button.
         \opt{HAVEREMOTEKEYMAP}{& \PluginRCUp{} / \PluginRCDown}
         & Adjust volume \\
 
-    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,SANSA_E200_PAD}{
+    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,SANSA_E200_PAD,SAMSUNG_YH820_PAD}{
       \ButtonRec
         \opt{HAVEREMOTEKEYMAP}{& }
         & Sync tap \\}
@@ -103,7 +103,7 @@ is different to enable navigation in the programmed track.
         \opt{HAVEREMOTEKEYMAP}{& \PluginRCUp{} / \PluginRCDown}
         & Adjust volume \\
 
-    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,SANSA_E200_PAD}{
+    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,SANSA_E200_PAD,SAMSUNG_YH820_PAD}{
       \ButtonRec
         \opt{HAVEREMOTEKEYMAP}{& }
         & Sync tap \\}
-- 
cgit v1.2.3

