From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/midiplay.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/plugins/midiplay.tex')

diff --git a/manual/plugins/midiplay.tex b/manual/plugins/midiplay.tex
index 6d28f71536..938762a88a 100644
--- a/manual/plugins/midiplay.tex
+++ b/manual/plugins/midiplay.tex
@@ -51,7 +51,8 @@ might experience ``Buffer miss!'' with many files, except simple ones.}
     \opt{GIGABEAT_PAD,GIGABEAT_S_PAD,SANSA_E200_PAD,SANSA_C200_PAD,SANSA_CLIP_PAD,IAUDIO_X5_PAD%
         ,IRIVER_H10_PAD,MROBE100_PAD,COWON_D2_PAD,SANSA_FUZEPLUS_PAD}{\ButtonPower}
     \opt{SANSA_FUZE_PAD}{Long \ButtonHome}
-    \opt{PBELL_VIBE500_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRec}
+    \opt{PBELL_VIBE500_PAD}{\ButtonRec}
+    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{Long \ButtonPlay}
     \opt{MPIO_HD200_PAD}{\ButtonRec + \ButtonPlay}
     \opt{MPIO_HD300_PAD}{Long \ButtonMenu}
        \opt{HAVEREMOTEKEYMAP}{& }
-- 
cgit v1.2.3

