From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/pegbox.tex | 13 ++++++++-----
 1 file changed, 8 insertions(+), 5 deletions(-)

(limited to 'manual/plugins/pegbox.tex')

diff --git a/manual/plugins/pegbox.tex b/manual/plugins/pegbox.tex
index cee50dd202..f82d0644c8 100644
--- a/manual/plugins/pegbox.tex
+++ b/manual/plugins/pegbox.tex
@@ -54,7 +54,7 @@ block and crosses which allow you to choose a replacement block.
     \opt{MPIO_HD200_PAD}{\ButtonRec}
     \opt{MPIO_HD300_PAD}{\ButtonMenu}
     \opt{SANSA_FUZEPLUS_PAD}{\ButtonBack}
-    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
+    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonFF}
     \opt{touchscreen}{\TouchTopRight}
         &
     \opt{HAVEREMOTEKEYMAP}{
@@ -74,7 +74,8 @@ block and crosses which allow you to choose a replacement block.
     \opt{COWON_D2_PAD}{\TouchBottomLeft}
     \opt{PBELL_VIBE500_PAD}{\ButtonOK}
     \opt{MPIO_HD200_PAD}{\ButtonPlay + \ButtonFF}
-    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonPlay+\ButtonFF}
+    \opt{SAMSUNG_YH92X_PAD}{\ButtonPlay+\ButtonUp}
+    \opt{SAMSUNG_YH820_PAD}{\ButtonRec+\ButtonUp}
         &
     \opt{HAVEREMOTEKEYMAP}{
         &}
@@ -92,8 +93,9 @@ block and crosses which allow you to choose a replacement block.
         \opt{MROBE100_PAD}{\ButtonDisplay}
         \opt{touchscreen}{\TouchBottomRight}
         \opt{PBELL_VIBE500_PAD}{\ButtonCancel}
-        \opt{MPIO_HD200_PAD}{\ButtonPlay + \ButtonRew}
-        \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonPlay+\ButtonRew}
+        \opt{MPIO_HD200_PAD}{\ButtonPlay{} + \ButtonRew}
+        \opt{SAMSUNG_YH92X_PAD}{\ButtonPlay+\ButtonDown}
+        \opt{SAMSUNG_YH820_PAD}{\ButtonRec+\ButtonDown}
             &
         \opt{HAVEREMOTEKEYMAP}{
             &}
@@ -108,7 +110,8 @@ block and crosses which allow you to choose a replacement block.
         ,SANSA_C200_PAD,SANSA_CLIP_PAD,COWON_D2_PAD,SANSA_FUZEPLUS_PAD}{\ButtonPower}
     \opt{SANSA_FUZE_PAD}{Long \ButtonHome}
     \opt{GIGABEAT_S_PAD}{\ButtonBack}
-    \opt{PBELL_VIBE500_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRec}
+    \opt{PBELL_VIBE500_PAD}{\ButtonRec}
+    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRew}
     \opt{MPIO_HD200_PAD}{\ButtonRec + \ButtonPlay}
     \opt{MPIO_HD300_PAD}{Long \ButtonMenu}
         &
-- 
cgit v1.2.3

