From 964a5e6dfb73983cfd5a14ed9e1af266cf4f9485 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Tue, 9 Aug 2011 14:39:32 +0000
Subject: Manual: A few more spelling corrections.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@30273 a1c6a512-1295-4272-9138-f99709370657
---
 manual/plugins/resistor.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/plugins/resistor.tex')

diff --git a/manual/plugins/resistor.tex b/manual/plugins/resistor.tex
index 27cc9a3e5e..2ae22dd862 100644
--- a/manual/plugins/resistor.tex
+++ b/manual/plugins/resistor.tex
@@ -23,6 +23,6 @@ an LED safely at a given voltage. First, select the voltage that the LED will
 use (the first option is the most common and a safe bet), and the current
 that it will draw (likewise with the first option). Then, use the onscreen
 keyboard to type in the supply voltage and, if selected, the custom 
-foreward current. This function produces safe estimates, but use your own
+forward current. This function produces safe estimates, but use your own
 judgement when using these output values. Power rating and displayed resistance
 are rounded up to the nearest common value.
-- 
cgit v1.2.3

