From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/rockboy.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/plugins/rockboy.tex')

diff --git a/manual/plugins/rockboy.tex b/manual/plugins/rockboy.tex
index 6eafbcb234..abb455c08b 100644
--- a/manual/plugins/rockboy.tex
+++ b/manual/plugins/rockboy.tex
@@ -101,7 +101,8 @@ the gnuboy emulator. To start a game, open a ROM file saved as \fname{.gb} or
     \opt{GIGABEAT_PAD,GIGABEAT_S_PAD,COWON_D2_PAD,PBELL_VIBE500_PAD%
         ,MPIO_HD300_PAD}{\ButtonMenu}
     \opt{SANSA_FUZEPLUS_PAD}{\ButtonBack}
-    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRec}
+    \opt{SAMSUNG_YH92X_PAD}{\ButtonRecOn}
+    \opt{SAMSUNG_YH820_PAD}{\ButtonRec}
        \opt{HAVEREMOTEKEYMAP}{& }
     & Open Rockboy menu\\
 \end{btnmap}
-- 
cgit v1.2.3

