From 25949f9cd10583d2e8907860851b0fa3c7280a72 Mon Sep 17 00:00:00 2001
From: Robert Kukla <roolku@rockbox.org>
Date: Wed, 5 Mar 2008 01:04:14 +0000
Subject: document dual-boot feature on m:robe 100

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@16524 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 15 +++++++++++++--
 1 file changed, 13 insertions(+), 2 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 1326db8787..0daff16549 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -268,7 +268,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{IPOD_4G_PAD,IPOD_3G_PAD}{\ButtonMenu{} / \ButtonSelect}%
       \opt{ONDIO_PAD}{\ButtonOff}\opt{RECORDER_PAD,PLAYER_PAD}%
           {Long \ButtonOn}%
-      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD}
+      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD}
           {\ButtonPower}%
       & Start Rockbox\\
       \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{Long \ButtonOff}%
@@ -276,7 +276,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{ONDIO_PAD,recorderv2fm}{Long \ButtonOff}%
       \opt{recorder}{Double tap \ButtonOff\ when playback is stopped}%
       \opt{PLAYER_PAD}{From the Main Menu, select \textbf{Shutdown}}%
-      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD}%
+      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD}%
           {Long \ButtonPower}%
       & Shutdown Rockbox\\
     \end{btnmap}
@@ -340,6 +340,17 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     Rockbox has a dual-boot feature. To boot into the original firmware,
     press and hold the \ButtonLeft{} button while turning on the player.
     }
+
+  \opt{mrobe100}
+    {
+    Rockbox has a dual-boot feature. It loads the original firmware from
+    the file \fname{/System/OF.mi4}. To boot into the original firmware,
+    when the \dap{} is turned off, press the \ButtonPower{} button once and then 
+    a second time when the m:robe bootlogo (the headphone) appears. Hold the
+    \ButtonPower{} button until you see the ``Loading original firmware...'' 
+    message on the screen.
+    }
+
   }
 
 \subsection{The first contact}
-- 
cgit v1.2.3

