From 4add1af7637e34567c5dedd6acfee3ccc4c0e8ac Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Tue, 6 Jan 2009 11:35:47 +0000
Subject: A couple of small fixes for the gigabeat s manual.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19698 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 28 +++++++++++++++-------------
 1 file changed, 15 insertions(+), 13 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index b9da763e9f..985fdf58b2 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -228,27 +228,29 @@ described in detail in the following paragraph.
   down to turn the \dap{} on or off.}
   %
   \opt{gigabeats}{
-  Hold the \dap{} with the screen on top and the controls on the right hand side.  
-  Below the screen is a cross-shaped pad which contains the \ButtonUp{}, 
-  \ButtonDown{}, \ButtonLeft{}, \ButtonRight{} and \ButtonSelect{} controls. 
-  On the top of the unit from left to right are the headphone socket and the 
+  Hold the \dap{} with the screen on top and the controls on the right hand side.
+  Directly below the bottom edge of the screen are two buttons, \ButtonBack{}
+  on the left and \ButtonMenu{} on the right. Below them is a cross-shaped pad
+  which contains the \ButtonUp{}, \ButtonDown{}, \ButtonLeft{}, \ButtonRight{}
+  and \ButtonSelect{} controls.
+  On the top of the unit from left to right are the headphone socket and the
   \ButtonHold{} switch.  The \ButtonHold{} switch puts the \dap{} into
-  hold mode when it is switched to the right of the unit. 
-  The buttons will have no effect when this is the case.  
-  
+  hold mode when it is switched to the right of the unit.
+  The buttons will have no effect when this is the case.
+
   Starting from the left hand side on the bottom of the unit, nearer to the back
-  than the front, is a recessed switch which controls whether the battery is on 
-  or off.  When this switch is to the left, the battery is disconnected.  
-  This can be used for a hard reset of the unit, or if the \dap{} is being placed 
+  than the front, is a recessed switch which controls whether the battery is on
+  or off.  When this switch is to the left, the battery is disconnected.
+  This can be used for a hard reset of the unit, or if the \dap{} is being placed
   in storage.  Next to that is a custom connector, presumably for planned accessories
   which were never released, and finally on the right hand side of the bottom of the
   unit is a mini USB socket for connecting directly to USB.
-  
+
   Finally on the right hand side of the unit are some control buttons.  Going from
-  the bottom of the unit to the top there are three small round buttons, the 
+  the bottom of the unit to the top there are three small round buttons, the
   \ButtonNext{} buttton, \ButtonPlay{} button, and \ButtonPrev{} button (from bottom
   to top) then a rocker volume switch with of the \ButtonVolDown{} button below the
-  \ButtonVolUp{} button.  Above that is one more small round button, the \ButtonPower{} 
+  \ButtonVolUp{} button.  Above that is one more small round button, the \ButtonPower{}
   button, which is held down to turn the \dap{} on or off.}
   %
   \opt{mrobe100}{
-- 
cgit v1.2.3

