From 4bbc9f68eae58180d6249e19697b5de30148da31 Mon Sep 17 00:00:00 2001
From: Marcin Bukat <marcin.bukat@gmail.com>
Date: Thu, 26 Jan 2012 10:11:18 +0100
Subject: MPIOs: manual work

Change-Id: Ief46eabf3611d6d21594f52f73292f2be5831b87
---
 manual/rockbox_interface/main.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 716cb824aa..ea5ad71059 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -536,7 +536,7 @@ detail in the following paragraph.
 To turn on and off your Rockbox enabled \dap{} use the following keys:
     \begin{btnmap}
       \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOn}%
-      \opt{MPIO_HD200_PAD}{Long \ButtonPlay}%
+      \opt{MPIO_HD200_PAD,MPIO_HD300_PAD}{Long \ButtonPlay}%
       \opt{IPOD_4G_PAD}{\ButtonMenu{} / \ButtonSelect}%
       \opt{IPOD_3G_PAD}{\ButtonMenu{} / \ButtonPlay}%
       \opt{ONDIO_PAD}{\ButtonOff}\opt{RECORDER_PAD,PLAYER_PAD}%
@@ -555,7 +555,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
           \\
 
       \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{Long \ButtonOff}%
-      \opt{MPIO_HD200_PAD}{Long \ButtonPlay}%
+      \opt{MPIO_HD200_PAD,MPIO_HD300_PAD}{Long \ButtonPlay}%
       \opt{IPOD_4G_PAD,IPOD_3G_PAD}{Long \ButtonPlay}%
       \opt{ONDIO_PAD,recorderv2fm}{Long \ButtonOff}%
       \opt{recorder}{Double tap \ButtonOff\ when playback is stopped}%
@@ -592,7 +592,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   {\ButtonPower} until the \dap{} shuts off or reboots.
 }%
 \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_M3_PAD,IRIVER_H10_PAD,MROBE100_PAD
-,PBELL_VIBE500_PAD,MPIO_HD200_PAD}{%
+,PBELL_VIBE500_PAD,MPIO_HD200_PAD,MPIO_HD300_PAD}{%
   In the unlikely event of a software failure, a hardware reset can be
   performed by inserting a paperclip gently into the Reset hole.
 }%
@@ -640,7 +640,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     and then press the \ButtonOn{} button.
     }
 
-  \opt{mpiohd200}
+  \opt{mpiohd200,mpiohd300}
     {
     Rockbox has a dual-boot feature. To boot into the original firmware,
     when the \dap{} is turned off, press and hold the \ButtonRec{} button,
-- 
cgit v1.2.3

