From 4c745fe8ac2a74262fbea038f7056e2f376734f0 Mon Sep 17 00:00:00 2001
From: Solomon Peachy <pizza@shaftnet.org>
Date: Sun, 22 Aug 2021 07:51:37 -0400
Subject: xduoox3: A few manual improvements

 * Fix a typo in a URL
 * Note how to enter the OF from the bootloader
 * Document how to perform a hard reset

Change-Id: I96d0d64cbd251573e1c5c55657ee5c5db510d9a6
---
 manual/rockbox_interface/main.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 16931e8d24..45da828143 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -570,7 +570,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
 }%
 \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_M3_PAD,IRIVER_H10_PAD,MROBE100_PAD
     ,PBELL_VIBE500_PAD,MPIO_HD200_PAD,MPIO_HD300_PAD,SAMSUNG_YH92X_PAD%
-    ,SAMSUNG_YH820_PAD}{%
+    ,SAMSUNG_YH820_PAD,XDUOO_X3_PAD}{%
   In the unlikely event of a software failure, a hardware reset can be
   performed by inserting a paperclip gently into the Reset hole.
 }%
-- 
cgit v1.2.3

