From 5b47b89d16fe2cef7654dba1edaa5043196c9e14 Mon Sep 17 00:00:00 2001
From: Marianne Arnold <pixelma@rockbox.org>
Date: Mon, 16 Aug 2010 09:43:48 +0000
Subject: First step of completing the target rename in the manual. Some target
 specific options were already renamed in the rest of the source (e.g. see
 r23883) but not where they are actually set - in the platform files - leading
 to parts included or excluded incorrectly. The problem exists for more
 targets, this commit deals with the supported Iaudios first. Rename 'x5' to
 'iaudiox5' (do the same for 'm5' and 'm3'), fix small errors or add missing
 info related to them along the way, use more appropriate options and simplify
 code a bit where possible.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@27823 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 0e4ec9ab4a..8303b647ef 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -9,7 +9,7 @@
 % The extension is selected in the preamble, so no further \ifpdfoutput
 % is necessary.
 \includegraphics[height=8cm,width=10cm,keepaspectratio=true]{rockbox_interface/images/\specimg-front}
-\opt{m3}{% replace with HAVEREMOTEKEYMAP when the h100 file exists or change specimg
+\opt{iaudiom3}{% replace with HAVEREMOTEKEYMAP when the h100 file exists or change specimg
   \end{center}
   % spacing between the two pictures, could possibly be improved
   \begin{center}
@@ -300,7 +300,7 @@ detail in the following paragraph.
   bottom of the unit, there is a connector for the docking station or the 
   proprietary USB connector for connecting directly to USB.}
   %
-  \opt{x5,m5}{
+  \opt{iaudiom5,iaudiox5}{
   The \dap{} is curved so that the end with the screen on it is thicker than the 
   other end.  Hold the \dap{} wih the thick end towards the top and the screen
   facing towards you.  Half way up the front of the unit on the right hand side
@@ -325,8 +325,8 @@ detail in the following paragraph.
   indicator light, which may feel a bit like a button, but is not.
   
   From the top of the \dap{} on the left hand side is the headphone socket, then the 
-  remote connector.  Below this is a cover which protects the \opt{x5}{USB host
-  connector.}\opt{m5}{USB and charging connector}.}
+  remote connector.  Below this is a cover which protects the \opt{iaudiox5}{USB
+  host connector.}\opt{iaudiom5}{USB and charging connector}.}
   %
   \opt{e200,e200v2}{
   Hold the \dap{} with the turning wheel at the front and bottom.  On the bottom left
@@ -555,7 +555,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   performed by inserting a paperclip gently into the Reset hole.
 }%
 
-\nopt{gigabeatf,m3,m5,x5,archos}
+\nopt{gigabeatf,iaudiom3,iaudiom5,iaudiox5,archos}
   {
   \subsection{Starting the original firmware}
   \label{ref:Dualboot}
-- 
cgit v1.2.3

