From 87b8e6bcee90c025e7ebd020faec8e00307691c0 Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Sat, 29 Jul 2006 09:30:56 +0000
Subject: fixed description of hard poweroff for ondio, removed A-B repeat from
 ondio manual, made more use of setting macro and broke some long lines.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@10358 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 3d737a5d81..9f991e8298 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -69,13 +69,13 @@ To turn on and shut down your \dap, the following keys are used:
     \end{btnmap}
 \end{table}
 \label{ref:Safeshutdown}On shutdown, Rockbox automatically saves its settings.
-
 \opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD}{
   In the unlikely event of a software failure, a hardware power off can be
-  performed by holding down 
+  performed by holding down
   \opt{PLAYER_PAD}{\ButtonStop}
   \opt{RECORDER_PAD,ONDIO_PAD}{\ButtonOff}
-  until the Jukebox power light goes off.
+  until the \nopt{ondiosp,ondiofm}{\dap\ power light}
+  \opt{ondiosp,ondiofm}{\daps\ display goes off}.
 }
 
 \section{\label{ref:file_browser}File Browser}
-- 
cgit v1.2.3

