From 8951024a67a33ab5cc36c80d932e09e818144787 Mon Sep 17 00:00:00 2001
From: Barry Wardell <rockbox@barrywardell.net>
Date: Wed, 21 Mar 2007 00:54:17 +0000
Subject: Explain how to get from the OF back to Rockbox on H10. Also explain
 about the Music folder being hidden on MTP models.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@12871 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 4 ++++
 1 file changed, 4 insertions(+)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index aa75d7d04f..4c64224d08 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -207,6 +207,10 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     {
     Rockbox has a dual-boot feature.  To boot into the original firmware, 
     press and hold the \ButtonRew{} button while turning on the player.
+    \note{The iriver firmware doesn't shut down properly when you turn it off, 
+    it only goes to sleep. To get back into Rockbox when exiting from the 
+    iriver firmware, you will need to reset the player by \opt{h10}{inserting a
+    pin in the reset hole}\opt{h10_5gb}{taking out battery}.}
     }
   }
 
-- 
cgit v1.2.3

