From 8a148d2c236f646d0c68d63a61084d97fd400f89 Mon Sep 17 00:00:00 2001
From: Dave Chapman <dave@dchapman.com>
Date: Tue, 13 Oct 2009 20:27:57 +0000
Subject: Changes to build a Nano2G manual.  It is now just missing the
 ipodnano2g-front.* images

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@23160 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 102e138d42..c58f3e68c7 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -156,7 +156,7 @@ described in detail in the following paragraph.
   \ButtonHold{} is off before trying to use your player. 
   }
   %
-  \opt{ipodnano}{
+  \opt{ipodnano,ipodnano2g}{
   The main controls on the \dap{} are a slightly indented wheel with a
   flat round button in the center. Hold the \dap{} with these controls on the
   top surface. There is a \ButtonHold{} switch at one end, and
@@ -480,7 +480,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   {
   \subsection{Starting the original firmware}
   \label{ref:Dualboot}
-  \opt{ipod4g,ipodcolor,ipodvideo,ipodnano,ipodmini}
+  \opt{ipod4g,ipodcolor,ipodvideo,ipodnano,ipodnano2g,ipodmini}
     {
     Rockbox has a dual-boot feature. To boot into the original firmware, shut
     down the device as described above. Turn on the \ButtonHold{} switch
-- 
cgit v1.2.3

